Pedestrian and Bicycle

AASHTO LRFD Bridge Design Specifications

FDOT Structures Design Guidelines

FDOT Structures Standard Drawings

Plans Preparation Manual - English (Volume I)

Standard Specifications for Road and Bridge Construction

AASHTO LRFD Bridge Design Specifications

13.4 General

13.5 Materials

13.6 Limit States and Resistance Factors

13.8 Pedestrian Railings

13.9 Bicycle Railings

13.10 Combination Railings

FDOT Structures Design Guidelines

1.4.1 Concrete Cover

2.5 Miscellaneous Loads

2.8 Barrier/Railing Distribution for Beam-Slab Bridges

Chap. 9 Bridge Cost Estimating

FDOT Structures Standard Drawings

720 Traffic Railing Barrier – (42” Vertical Shape) DGN | DGN | PDF

730 Traffic Railing Barrier – (32” Vertical Shape) DGN | DGN | PDF

771 Traffic Railing Barrier – (Thrie Beam Retrofit) General Notes & Details DGN | DGN | PDF

800 Pedestrian/Bicycle Railing DGN | PDF

810 Aluminum Pedestrian/Bicycle Bullet Railing for Traffic Railing Barrier (32” F-Shape) DGN | PDF

820 Aluminum Pedestrian/Bicycle Bullet Railing Details DGN | DGN | PDF

850 Steel Pedestrian/Bicycle Picket Railing DGN | DGN | PDF

860 Aluminum Pedestrian/Bicycle Picket Railing DGN | DGN | PDF

870 Aluminum Pipe Guiderail DGN | PDF

Plans Preparation Manual – English (Volume I)

2.12 Bridge Railing and Separators

Chap. 8 Pedestrian and Bicycle Facilities

For current Plans Preparation Manual:

http://www.dot.state.fl.us/rddesign/PPM Manual/PPM.htm

Standard Specifications for Road and Bridge Construction

Section 346 Portland Cement Concrete

Section 400 Concrete Structures

Section 415 Reinforcing Steel

Section 515 Pipe Handrail

Section 965 General Provisions for Aluminum Items (Including Welding)

For current specifications: http://www.dot.state.fl.us/specificationsoffice/