Structures Design Guidelines | Jan 2008
3 - Substructure and Retaining Walls |

## 3.13 Retaining Wall Design

### 3.13.1 General

A. Use Chapter 30, Plans Preparation Manual for retaining wall plans preparation and administrative requirements in conjunction with the design requirements of this Section. Refer to SDG Chapter 1 for the retaining wall concrete class
(excluding MSE Walls) and reinforcing steel cover requirements
.

B. Rankine earth pressure may be used in lieu of lateral earth loads on walls developed from Coulomb earth pressure. If Rankine earth pressure is used, the resultant lateral earth load can be assumed to be located at the centroid of the earth pressure diagram.

C. During the design process, review wall locations for conflicts with existing or proposed utilities located beneath proposed reinforced fill wall volume. Analyze for settlement effects, maintenance repair access, etc.

D. Do not place utilities in the soil-reinforced zone behind Mechanically Stabilized Earth (MSE) or tie-back walls.

Commentary:Utilities placed below the wall or in the reinforced zone cannot be maintained because excavation in this zone will compromise the structural integrity of these wall types. Leaking pipes could wash out and destroy the structural integrity of the wall.

### 3.13.2 Mechanically Stabilized Earth Walls [11.10] (07/07) July 2007 - Renumbered sections B. through L. Revised I- Apparent Coefficient of Friction, changed E. and H. from "H1 = mechanical wall height" to "H = height of wall". Added H.5- reference to External Stability Analysis software.

Commentary: FHWA Publication No. FHWA-NHI-00-043, “Mechanically Stabilized Earth Walls and Reinforced Soil Slopes Design & Construction Guidelines”, contains background information on the initial development of MSE wall design and is referenced by LRFD Article 11.10.1 as the design guidelines for geometrically complex MSE walls.

A. For MSE Walls, use the following Table for concrete class and cover requirements:

Distance (D)1 | Concrete | Cover
D > 2,500 feet (low air contaminants) | Class II | 2-inches
2,500 feet >= D >= 300 feet (moderate air contaminants) | Class IV | 2-inches
D < 300 feet (extreme air contaminants)2 | Class IV | 3-inches
1- Distance (D) from wall to a body of water with high chloride content (greater than 2,000 ppm) or any coal burning industrial facility, pulpwood plant, fertilizer plant or similar industry. 2- Include calcium nitrite when D <= 50 feet (splash zone).

B. Minimum Service Life [11.5.1]

1.) Design permanent walls for a service life of 75 years, except those supporting abutments on spread footings. Design walls supporting abutments on spread footings for a service life of 100 years.

2.) Design temporary walls for the length of contract or a service life of three years, whichever is greater.

C. Concrete Leveling Course

1.) All permanent walls will have a non-structural concrete leveling course as a minimum.

2.) The entire bottom of the wall panel will have bearing on the concrete leveling course.

D. Bin Walls [11.10.1]

1.) When two walls intersect forming an internal angle of less than 70 degrees, design the nose section as a bin wall. Submit calculations for this special design with the plans for review and approval.

2.) Design structural connections between wall facings within the nose section to create an at-rest bin effect without eliminating flexibility of the wall facings to allow tolerance for differential settlements.

3.) For wall facings without continuous vertical open joints, such as square or rectangular panels, design the nose section to settle differentially from the remainder of the structure with a slip joint. Facing panel overlap, interlock or rigid connection across vertical joints is not permitted.

4.) Design soil reinforcements to restrain the nose section by connecting directly to each of the facing elements in the nose section. Run soil reinforcement into the backfill of the main reinforced soil volume to a plane at least 3 feet beyond the Coulomb (or Rankine) failure surface (See Figure 3-18).

5.) Design of facing connections, pullout and strength of reinforcing elements and obstructions must conform to the general requirements of the wall design.

E. Minimum Length of Soil Reinforcement [11.10.2.1]

In lieu of the requirements for minimum soil reinforcement lengths in LRFD Article [C11.10.2.1] and substitute the following:

The minimum soil reinforcement length, “L”, measured from the back of the facing element, must be the maximum of the following:

Walls in Front of Abutments on Piling L ≥ 8 feet and L ≥ 0.7H

Walls Supporting Abutments on Spread Footings L ≥ 22 feet and L ≥ 0.6 ( H + d ) + 6.5 feet, ( d = fill height above wall ) and L ≥ 0.7 H

Where: H = height of wall, in feet, and measured from the top of the leveling pad to the top of the wall coping. L = length in feet, required for external stability design.

Commentary: As a rule of thumb, for a MSE wall with reinforcement lengths equal to 70% of the wall height, the anticipated factored bearing pressure (quniform) can be estimated to be about 200% of the overburden weight of soil and surcharge. It may be necessary to increase the reinforcement length for external stability to assure that the factored bearing pressure does not exceeds the factored bearing resistance (qr) of the foundation soil at this location.

F. Minimum Front Face Wall Embedment [11.10.2.2]

1.) Consider scour and bearing capacity when determining front face embedment depth.

2.) Consult the District Drainage and Geotechnical Engineers to determine the elevation of the top of leveling pad.

3.) In addition to the requirements for minimum front face embedment in LRFD Article [11.10.2.2], the minimum front face embedment for permanent walls must comply with both a minimum of 24-inches to the top of the leveling pad and Figure 3-19. Also, consider normal construction practices.

G. Facing [11.10.2.3]

1.) The typical panel size must be square and not exceed 30 square feet in area (5 feet by 5 feet, nominal).

2.) The typical non-square (i.e., diamond shaped, not rectangular) panel size must not exceed 40 square feet in area.

3.) Special panels (top out, etc.) must not exceed 50 square feet in area.

4.) Full-height facing panels must not exceed 8 feet in height.

5.) SDO will consider use of larger panels on a case-by-case basis. The reinforcing steel concrete cover must comply with Table in 3.13.2.A.

H. External Stability [11.10.5] The reinforced backfill soil parameters for analysis are:

1.) Sand Backfill (Statewide except Miami-Dade and Monroe Counties).

a.) Moist Unit Weight: 105 lbs per cubic foot.

b.) Friction Angle: 30 degrees

2.) Limerock Backfill (Miami-Dade and Monroe Counties only).

a.) Moist Unit Weight: 115 lbs per cubic foot.

b.) Friction Angle: 34 degrees.

3.) In addition to the horizontal back slope with traffic surcharge figure in LRFD, Figure 3-16 illustrates a broken back slope condition with a traffic surcharge. If a traffic surcharge is present and located within 0.5H of the back of the reinforced soil volume, then it must be included in the analysis. Figure 3-17 illustrates a broken back slope condition without a traffic surcharge.

4.) The Geotechnical Engineer of Record for the project is responsible for designing the reinforcement lengths for the external conditions shown in Figure 3-1 and any other conditions that are appropriate for the site.

5.) See Volume 7 - Design Aids for the LRFD External Stability Analysis for MSE Walls (v2.5).

I. Apparent Coefficient of Friction [11.10.6.3.2] The pullout friction factor (F*) and the resistance factor for pullout (Ø) need not be modified for the design of soil reinforcement below the design flood elevation.

J. Soil Reinforcement Strength [11.10.6.4]

1.) In lieu of the corrosion rates specified in LRFD Article [11.10.6.4.2a], substitute the following requirements: The following corrosion rates for metallic reinforcement apply to non-corrosive environments only (low and moderate air contaminants in Table 3.13.2.A):

a.) Zinc (first 2 years) 0.59 mils/year

b.) Zinc (subsequent years to depletion) 0.16 mils/year

c.) Carbon Steel (after depletion of zinc) 0.48 mils/year

d.) Carbon Steel (75 to 100 years) 0.28 mils/year

2.) Use a minimum corrosion rate of 6 mils/year for Temporary MSE Walls with: a.) metallic reinforcement below the 100 year flood elevation. b.) wire facing and connections exposed to extreme air contaminants (Table 3.13.2.A).

3.) Do not use metal soil reinforcement if the wall is located within the 100 year flood plain and the nearby water chloride content is greater than 2,000 ppm.

4.) Epoxy coated reinforcement mentioned in LRFD Commentary [C11.10.6.4.2a] is not permitted. Passive metal soil reinforcement (i.e., stainless steel, aluminum alloys, etc.), is permitted only with written SDO approval.

5.) Geosynthetic reinforcements (LRFD 11.10.6.4.2b) must comply with Chapter 31 of the Plans Preparation Manual, Volume I. Use the same reinforcement properties as those for geosynthetic reinforced soil slopes shown on Design Standards Index No. 501 with a maximum 2% strain for permanent walls and 5% strain for temporary walls.

6.) For geosynthetic reinforcement, supplement LRFD Table 11.10.6.4.3b-1 with the following default value:

Application | Total Reduction Factor, RF
Critical temporary wall applications with non-aggressive soils and polymers meeting the requirements listed in Table 11.10.6.4.2b-1. | 7.0

7.) For permanent wall systems using welded wire soil reinforcement, the minimum wire size in both the longitudinal and transverse directions shall be W10 for walls with a 75-year service life and W11 for walls with a 100-year service life.

8.) Do not design soil reinforcement to be skewed more than 15 degrees from a position normal to the wall panel unless necessary and clearly detailed for acute corners. In these instances, follow the pre-approved bin wall details shown in the QPL Vendor Drawings.

Commentary: There are times when the 15 degree criteria cannot be met due to vertical obstructions such as piling, drainage structures or bridge obstructions with angles. In these cases, clearly detail the soil reinforcement skew details in the Shop Drawings.

9.) Do not design soil reinforcement to be skewed more than 15 degrees from a horizontal position in elevation view to clear horizontal obstructions.

10.) Soil reinforcement must not be attached to piling, and abutment piles must not be attached to any retaining wall system.

K. Reinforcement/Facing Connection [11.10.6.4.4] Design the soil reinforcement to facing panel connection to assure full contact of the connection elements. The connection must be able to be inspected visibly during construction.

Commentary: Normally mesh and bar mats are connected to the facing panel by a pin passing through loops at the end of the reinforcement and loops inserted into the panels. If these loops are not aligned, then some reinforcement will not be in contact with the pins causing the remaining reinforcement to be unevenly stressed and/or over stressed. If the quality of this connection cannot be assured through pullout testing and quality control during installation, then the strength of the soil reinforcement and its connections should be reduced accordingly.

L. End Bents on Piling behind MSE Walls

1.) All end bent piles must be plumb when MSE Wall is not parallel to the end bent centerline.

2.) The minimum clear distance shall be 24-inches for both of the following:

a.) Between the front face of the end bent cap or footing and the back face of wall panel.

b.) Between the face of piling and leveling pad. (The 24-inch dimension is based on the use of 18-inch piles. Whenever possible for larger piles, increase the clear distance between the wall and pile such that no soil reinforcement is skewed more than 15 degrees).

3.) Soil reinforcement to resist the overturning produced by the earth load, friction, and temperature must be attached to end bents, unless the long-term settlement exceeds 4-inches. In this case, the reinforcement must not be attached to the end bent and a special wall behind the backwall must be designed to accommodate the earth load.

M. End Bents on Spread Footings behind MSE Walls:

1.) The spread footing must be sized so that the factored bearing pressure does not exceed 6,000 psf.

2.) The edge of the footing must be a minimum of 12-inches behind the back of the wall panel.

3.) The minimum distance between the centerline of bearing on the end bent and the back of the wall panel must be 48-inches.