Pedestrian and Bicycle

AASHTO LRFD Bridge Design Specifications

FDOT Structures Design Guidelines

FDOT Structures Standard Drawings

Plans Preparation Manual - English (Volume I)

Standard Specifications for Road and Bridge Construction

AASHTO LRFD Bridge Design Specifications
13.4 | General
13.5 | Materials
13.6 | Limit States and Resistance Factors
13.8 | Pedestrian Railings
13.9 | Bicycle Railings
13.10 | Combination Railings

FDOT Structures Design Guidelines
1.4.2 | Concrete Cover
2.5 | Miscellaneous Loads
2.8 | Barrier/Railing Distribution for Beam-Slab Bridges
Chap. 9 | Bridge Cost Estimating

FDOT Structures Standard Drawings
422 | Traffic Railing – (42” Vertical Shape)
423 | Traffic Railing – (32” Vertical Shape)
470 | Traffic Railing – (Thrie Beam Retrofit) General Notes & Details
820 | Pedestrian/Bicycle Railing
821 | Aluminum Ped/Bicycle Bullet Railing for Traffic Railing (32” F-Shape)
822 | Aluminum Pedestrian/Bicycle Bullet Railing Details
850 | Steel Pedestrian/Bicycle Picket Railing
860 | Aluminum Pedestrian/Bicycle Picket Railing
870 | Aluminum Pipe Guiderail

Plans Preparation Manual – English (Volume I)
2.12 | Bridge Railing and Separators
Chap. 8 | Pedestrian and Bicycle Facilities
For current Plans Preparation Manual: http://www.fdot.gov/roadway/PPMManual/PPM.htm

Standard Specifications for Road and Bridge Construction
Section 346 | Portland Cement Concrete
Section 400 | Concrete Structures
Section 415 | Reinforcing Steel
Section 515 | Pipe Handrail
Section 965 | General Provisions for Aluminum Items (Including Welding)
For current specifications: http://www.dot.state.fl.us/specificationsoffice/