{"text_format":"1","workbook":"xlsx","n_sheets":8,"sheets":["Digital Signature-Instructions","Setup","FuelWS","Sheet2","Instructions - Pay Item adj's","Template","Accuracy","FuelFactors"],"not_rendered":{"charts":0,"images":13,"macros":1,"external_links":0,"defined_names":25,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Digital Signature-Instructions","index":0,"n_rows":137,"n_cols":3,"rows_kept":137,"cut":false,"hidden":false,"merged":[[82,2,82,14],[0,0,14,12],[16,1,16,14],[15,1,15,14],[62,2,62,12],[36,2,36,14]]}
["Prior to applying your digital signature in Excel, \nensure Calculation Options are set to Manual, then click Calculate Now."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Note:"]
[null,"If emailing this file, do not use the \"Share\" option in Excel. This will remove the digital signature/certificate. Instead, attach the digitally signed file to an email.\n\nTo save the attached file to an email, save using \"Drag and Drop\" or \"Right Click\" on the file and select \"Save As\". Otherwise, a new version of the document will be created, which will invalidate the digital signature."]
[]
["1.",null,"Save document (i.e., \"File\", \"Save As\"). Enter required information in the \"Setup Tab\"."]
[]
["2.",null,"Enter quantities in the \"FuelWS\" Tab as applicable."]
[]
["3.",null,"Select the \"View Signatures\" button in the \"Yellow ribbon\" above."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["4.",null,"The \"Signatures\" window will open. Select \"Contractor's Authorized Agent\". Then click on the drop arrow and select \"Sign…\""]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["5.",null,"Enter the name of the Contractor's Authorized Agent.\nOptional: Select \"Details...\" to enter contact information (i.e., address).\nSelect \"Sign\" to finalize digital signature."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["6.",null,"Notice that any edits done to the document after it has ben digitally signed will invalidate the signature certificate. The document will have to be created and signed again."]
[]
[]
[]
["7.",null,"View/access the signature after document has been digitally signed:"]
[]
[null,"a.","Select \"File\"."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"b.","Select \"View Signatures\"."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"c.","Select the drop down arrow and select \"Signature Details…\""]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"d.","Select the different options to see the desired signature details."]

{"sheet":"Setup","index":1,"n_rows":32,"n_cols":15,"rows_kept":32,"cut":false,"hidden":false,"merged":[[1,1,1,16],[2,1,2,16],[3,1,3,16],[4,10,4,12],[33,1,33,3],[27,6,27,15],[23,10,23,12],[23,14,23,15],[32,1,32,3],[30,1,30,3],[31,1,31,3],[11,5,11,15],[7,5,7,15],[7,2,7,3],[9,2,9,3],[9,5,9,15],[11,2,11,3],[13,2,13,3],[13,5,13,9],[13,10,13,12],[13,14,13,15],[17,3,17,8],[21,3,21,8],[17,14,17,15],[17,10,17,12],[19,10,19,12],[19,14,19,15],[21,14,21,15],[21,10,21,12],[19,3,19,8]]}
[]
[]
[null,"Contractor's Certification of Fuel Adjustment"]
[null,"(Design Build and Lump Sum Projects)"]
[null,null,null,null,null,"Worksheet No."]
[]
[]
[null,null,"Financial Project ID:"]
[]
[null,null,"Contractor:"]
[]
[null,null,"Contract Number:"]
[]
[null,null,"From (Mo/Day/Yr):",null,null,null,null,null,null,null,"To (Mo/Day/Yr):"]
[]
[]
[]
[null,null,null,"Month / Year",null,null,null,null,null,null,"Gasoline Index",null,null,null,"Diesel Index"]
[]
[null,null,"Base Index:"]
[]
[null,null,"Current Index:"]
[]
[null,null,"Index Difference:",null,null,null,null,null,null,null,{"$f":"IF((GasolineBaseIndex*1.05)<=GasolineCurrentIndex,GasolineCurrentIndex-(GasolineBaseIndex*1.05),IF((GasolineBaseIndex*0.95)>=GasolineCurrentIndex,GasolineCurrentIndex-(GasolineBaseIndex*0.95),0))","v":0},null,null,null,{"$f":"IF((DieselBaseIndex*1.05)<=DieselCurrentIndex,DieselCurrentIndex-(DieselBaseIndex*1.05),IF((DieselBaseIndex*0.95)>=DieselCurrentIndex,DieselCurrentIndex-(DieselBaseIndex*0.95),0))","v":0}]
[]
[]
[]
[]
[]
[]
[null,"Effective January 2013 Letting"]
[null,"(Revision 12/10/19)"]

{"sheet":"FuelWS","index":2,"n_rows":1127,"n_cols":14,"rows_kept":1127,"cut":false,"hidden":false,"merged":[[911,7,911,11],[1,2,1,13],[2,2,2,13],[905,0,905,3],[905,9,905,10],[907,0,907,9],[1025,3,1025,6],[908,0,908,2],[188,2,188,3],[215,2,215,3],[119,2,119,3],[120,2,120,3],[121,2,121,3],[122,2,122,3],[183,2,183,3],[184,2,184,3],[185,2,185,3],[186,2,186,3],[187,2,187,3],[131,2,131,3],[132,2,132,3],[133,2,133,3],[134,2,134,3],[135,2,135,3],[904,4,904,5],[254,2,254,3],[269,2,269,3],[261,2,261,3],[181,2,181,3],[182,2,182,3],[93,2,93,3],[94,2,94,3],[75,2,75,3],[189,2,189,3],[255,2,255,3],[256,2,256,3],[257,2,257,3],[258,2,258,3],[259,2,259,3],[128,2,128,3],[129,2,129,3],[130,2,130,3],[136,2,136,3],[272,2,272,3],[265,2,265,3],[197,2,197,3],[198,2,198,3],[137,2,137,3],[7,3,7,4],[5,3,5,4],[3,3,3,4],[9,7,11,8],[214,2,214,3],[190,2,190,3],[191,2,191,3],[192,2,192,3],[193,2,193,3],[199,2,199,3],[194,2,194,3],[195,2,195,3],[196,2,196,3],[51,2,51,3],[123,2,123,3],[124,2,124,3],[125,2,125,3],[126,2,126,3],[127,2,127,3],[9,1,11,1],[74,2,74,3],[12,2,12,3],[33,2,33,3],[118,2,118,3],[71,2,71,3],[72,2,72,3],[42,2,42,3],[43,2,43,3],[44,2,44,3],[45,2,45,3],[48,2,48,3],[50,2,50,3],[70,2,70,3],[9,2,11,3],[30,2,30,3],[52,2,52,3],[53,2,53,3],[270,2,270,3],[271,2,271,3],[273,2,273,3],[277,2,277,3],[260,2,260,3],[262,2,262,3],[263,2,263,3],[264,2,264,3],[297,2,297,3],[292,2,292,3],[293,2,293,3],[294,2,294,3],[295,2,295,3],[296,2,296,3],[274,2,274,3],[275,2,275,3],[276,2,276,3],[284,2,284,3],[285,2,285,3],[9,13,11,14],[9,11,11,12],[46,2,46,3],[41,2,41,3],[39,2,39,3],[9,5,11,6],[9,9,11,10],[37,2,37,3],[32,2,32,3],[34,2,34,3],[9,4,11,4],[903,11,903,14],[903,4,903,5],[278,2,278,3],[279,2,279,3],[280,2,280,3],[281,2,281,3],[287,2,287,3],[288,2,288,3],[289,2,289,3],[290,2,290,3],[291,2,291,3],[298,2,298,3],[299,2,299,3],[300,2,300,3],[306,2,306,3],[307,2,307,3],[308,2,308,3],[310,2,310,3],[311,2,311,3],[301,2,301,3],[302,2,302,3],[303,2,303,3],[304,2,304,3],[305,2,305,3],[321,2,321,3],[322,2,322,3],[323,2,323,3],[324,2,324,3],[325,2,325,3],[316,2,316,3],[317,2,317,3],[282,2,282,3],[283,2,283,3],[286,2,286,3],[309,2,309,3],[318,2,318,3],[319,2,319,3],[320,2,320,3],[312,2,312,3],[313,2,313,3],[314,2,314,3],[315,2,315,3],[331,2,331,3],[332,2,332,3],[333,2,333,3],[334,2,334,3],[335,2,335,3],[326,2,326,3],[327,2,327,3],[328,2,328,3],[329,2,329,3],[330,2,330,3],[341,2,341,3],[342,2,342,3],[343,2,343,3],[344,2,344,3],[345,2,345,3],[336,2,336,3],[337,2,337,3],[338,2,338,3],[339,2,339,3],[340,2,340,3],[364,2,364,3],[365,2,365,3],[366,2,366,3],[368,2,368,3],[369,2,369,3],[347,2,347,3],[348,2,348,3],[349,2,349,3],[350,2,350,3],[351,2,351,3],[910,7,910,11],[928,7,928,11],[268,2,268,3],[387,2,387,3],[388,2,388,3],[389,2,389,3],[390,2,390,3],[391,2,391,3],[382,2,382,3],[383,2,383,3],[384,2,384,3],[385,2,385,3],[386,2,386,3],[381,2,381,3],[372,2,372,3],[373,2,373,3],[374,2,374,3],[375,2,375,3],[376,2,376,3],[367,2,367,3],[397,2,397,3],[398,2,398,3],[399,2,399,3],[357,2,357,3],[400,2,400,3],[392,2,392,3],[393,2,393,3],[394,2,394,3],[54,2,54,3],[370,2,370,3],[371,2,371,3],[377,2,377,3],[378,2,378,3],[358,2,358,3],[359,2,359,3],[360,2,360,3],[361,2,361,3],[352,2,352,3],[353,2,353,3],[354,2,354,3],[355,2,355,3],[356,2,356,3],[395,2,395,3],[396,2,396,3],[379,2,379,3],[380,2,380,3],[362,2,362,3],[363,2,363,3]]}
[]
[null,null,"CONTRACTOR'S CERTIFICATION OF FUEL ADJUSTMENT"]
[null,null,"(DESIGN BUILD AND LUMP SUM PROJECTS) "]
[null,"CONTRACTOR:",{"$f":"ContractorName","v":0},"DATE FROM:",null,{"$f":"DateFrom","v":"00:00:00"},null,null,null,"MONTH / YEAR",null,"GASOLINE INDEX",null,"DIESEL INDEX"]
[]
[null,"WORKSHEET NO.:",{"$f":"CertificationNumber","v":0},"DATE TO:",null,{"$f":"DateTo","v":"00:00:00"},null,"BASE INDEX:",null,{"$f":"BaseIndexMonth","v":"00:00:00"},null,{"$f":"GasolineBaseIndex","v":0},null,{"$f":"DieselBaseIndex","v":0}]
[]
[null,"FINANCIAL PROJECT ID:",{"$f":"FinancialIDNumber","v":0},"CONTRACT NO.:",null,{"$f":"ContractNumber","v":0},null,"CURRENT INDEX:",null,{"$f":"CurrentIndexMonth","v":"00:00:00"},null,{"$f":"GasolineCurrentIndex","v":0},null,{"$f":"DieselCurrentIndex","v":0}]
[]
[null,"ITEM NUMBER(S)","ITEM DESCRIPTION",null,"UNIT","QUANTITY",null,"GASOLINE\n(GALLONS)",null,"DIESEL\n(GALLONS)",null,"GASOLINE\nFACTOR",null,"DIESEL\nFACTOR"]
[]
[]
[null,"0110-1-1 ","Clearing & Grubbing*",null,"LS/AC",null,null,{"$f":"ROUND(F13*L13,0)","v":0},null,{"$f":"ROUND(F13*N13,0)","v":0},null,25.272476000000001,null,251.47870800000001]
[null,"0110-2-1","Clearing & Grubbing",null,"AC",null,null,{"$f":"ROUND(F14*L14,0)","v":0},null,0,null,25.272476000000001,null,251.47870800000001]
[null,"0110-15","Arborist Work, Complete*",null,"LS/AC",null,null,{"$f":"ROUND(F15*L15,0)","v":0},null,0,null,25.272476000000001,null,251.47870800000001]
[null,"0110-20-1 ","Removal of Existing Wall/ MSE Wall*",null,"LS/SF",null,null,{"$f":"+ROUND(F16*L16,0)","v":0},null,0,null,25.272476000000001,null,251.47870800000001]
[null,"0110-20-2","Removal of Existing Wall/ Retaining Wall*",null,"LS/SF",null,null,0,null,0,null,25.272476000000001,null,251.47870800000001]
[null,"0110-4","Removal of Concrete Pavement",null,"SY",null,null,0,null,0,null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-3","Removal of Existing Concrete, Concrete Sidewalk and Driveways",null,"SY",null,null,0,null,{"$f":"ROUND(F19*N19,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-4","Removal of Existing Concrete, Slope Pavement",null,"SY",null,null,0,null,{"$f":"ROUND(F20*N20,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-5","Removal of Existing Concrete, Curb Elements",null,"SY",null,null,0,null,{"$f":"ROUND(F21*N21,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-6","Removal of Existing Concrete, Ditch Pavement",null,"SY",null,null,0,null,{"$f":"ROUND(F22*N22,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-7","Removal of Existing Concrete, Rigid Concrete Pavement",null,"SY",null,null,0,null,{"$f":"ROUND(F23*N23,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-10","Removal of Existing Concrete",null,"SY",null,null,{"$f":"+ROUND(F24*L24,0)","v":0},null,0,null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-11","Removal of Existing Concrete, Permanent Barrier Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F25*N25,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-12","Removal of Existing Concrete, MSE Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F26*N26,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-13","Removal of Existing Concrete, Retaining Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F27*N27,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-15","Removal of Existing Concrete, Perimeter Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F28*N28,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-16","Removal of Existing Concrete, Gravity Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F29*N29,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0110-4-17","Removal of Existing Concrete, Architectural/Decorative Wall",null,"SY",null,null,0,null,{"$f":"ROUND(F30*N30,0)","v":0},null,4.7100000000000003E-2,null,2.3409]
[null,"0120-1",{"$f":"VLOOKUP(B31,FuelFactorDataRange,2,FALSE)","v":"Regular Excavation"},null,{"$f":"VLOOKUP(B31,FuelFactorDataRange,3,FALSE)","v":"CY"},null,null,{"$f":"ROUND(F31*L31,0)","v":0},null,0,null,1.0466E-2,null,0.55122800000000005]
[null,"0120-1-900","Regular Excavation, Projects 405270-1,-3,and -4",null,"CY",null,null,{"$f":"ROUND(F32*L32,0)","v":0},null,0,null,1.0466E-2,null,0.29766300000000001]
[null,"0120-2-2","Borrow Excavation",null,"CY",null,null,{"$f":"ROUND(F33*L33,0)","v":0},null,0,null,1.3082999999999999E-2,null,0.823183]
[null,"0120-3","Lateral Ditch Excavation",null,"CY",null,321321,{"$f":"ROUND(F34*L34,0)","v":0},null,{"$f":"ROUND(F34*N34,0)","v":0},null,2.3026999999999999E-2,null,0.54687300000000005]
[null,"0120-4 ","Excavation Subsoil",null,"CY",null,321321,0,null,0,null,1.4205000000000001E-2,null,0.61934]
[null,"0120-4-900","Excavation Subsoil, Projects 405270-1,-3, and -4",null,"CY",null,null,0,null,0,null,1.4205000000000001E-2,null,0.39637800000000001]
[null,"0120-5","Channel Excavation",null,"CY",null,null,0,null,0,null,0.78500000000000003,null,0.58626699999999998]
[null,"0120-6","Embankment",null,"CY",null,321321,0,null,0,null,6.5420000000000001E-3,null,0.51722999999999997]
[null,"0120-6-900","Embankment, Projects 405270-1, -3, and-4",null,"CY",null,null,0,null,0,null,6.5420000000000001E-3,null,0.24826999999999999]
[null,"0160-4","Type B Stabilization",null,"SY",null,321321,0,null,0,null,1.1651E-2,null,0.47264899999999999]
[null,"0160-4-900","Type B Stabilization, Projects 405270-1,-3, and -4",null,"SY",null,null,0,null,0,null,1.1651E-2,null,0.25523000000000001]
[null,"0162-1-11","Prepared Soil Layer -Finish Soil, 6",null,"SY",null,321321,0,null,0,null,1.0907E-2,null,0.10748199999999999]
[null,"0162-1-12","Prepared Soil Layer -Finish Soil, 12",null,"SY",null,null,0,null,0,null,1.3082999999999999E-2,null,0.18313699999999999]
[null,"0162-1-21","Prepared Soil Layer -Organic Soil, 6",null,"SY",null,null,0,null,0,null,1.0907E-2,null,0.10748199999999999]
[null,"0162-1-22","Prepared Soil Layer -Organic Soil,12",null,"SY",null,null,0,null,0,null,1.3082999999999999E-2,null,0.18313699999999999]
[null,"0162-1-33","Prepared Soil Layer -Blanket, Special",null,"SY",null,null,{"$f":"ROUND(F46*L46,0)","v":0},null,0,null,1.3082999999999999E-2,null,0.18313699999999999]
[null,"0285-701 thru 285-708","Optional Base (Base Group 01 thru Group 08)",null,"SY",null,321321,{"$f":"ROUND(F47*L47,0)","v":0},null,0,null,1.2692999999999999E-2,1.2692999999999999E-2,0.69760800000000001]
[null,"0285-701-900","Optional Base Group 01, Projects 405270-1,-3, and -4",null,"SY",null,null,{"$f":"ROUND(F48*L48,0)","v":0},null,0,null,9.3860000000000002E-3,null,0.36104700000000001]
[null,"0285-709 thru 285-715","Optional Base (Base Group 09 thru Group 15)",null,"SY",null,null,{"$f":"ROUND(F49*L49,0)","v":0},null,0,null,2.0448000000000001E-2,2.0448000000000001E-2,1.280054]
[null,"0285-709-900","Optional Base Group 09, Projects 405270-1,-3, and -4",null,"SY",null,null,0,null,0,null,1.7585E-2,null,0.37234099999999998]
[null,"0285-701 thru 285-708","Optional Base (Base Group 01 thru 08)  (Asphalt Only)",null,"SY",null,null,0,null,0,null,9.0989999999999994E-3,9.0989999999999994E-3,3.1490230000000001]
[null,"0285-709 thru 285-715","Optional Base (Base Group 09 thru 15)  (Asphalt Only)",null,"SY",null,null,0,null,0,null,1.4629E-2,1.4629E-2,4.6982249999999999]
[null,"0285-722","Optional Base (16\" Graded Aggregate)",null,"SY",null,null,0,null,0,null,3.2024999999999998E-2,null,1.518281]
[null,"0285-730","Optional Base (16\" Graded Aggregate)",null,"SY",null,null,{"$f":"ROUND(F54*L54,0)","v":0},null,{"$f":"ROUND(F54*N54,0)","v":0},null,3.2024999999999998E-2,null,1.518281]
[null,"0285-731","Optional Base (18\" Graded Aggregate)",null,"SY",null,null,{"$f":"ROUND(F55*L55,0)","v":0},null,{"$f":"ROUND(F55*N55,0)","v":0},null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-732","Optional Base (16\" Graded Aggregate)",null,"SY",null,null,0,null,0,null,3.2024999999999998E-2,null,1.518281]
[null,"0285-733","Optional Base (18\" Graded Aggregate)",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-734","Optional Base (20\" Graded Aggregate)",null,"SY",null,null,0,null,0,null,4.1346000000000001E-2,null,1.920142]
[null,"0285-735","Optional Base (16\" Graded Aggregate) Project 421012-1-52-01",null,"SY",null,null,0,null,0,null,3.2024999999999998E-2,null,1.518281]
[null,"0285-736","Optional Base (24\" Graded Aggregate) Project 441322-2-52-01",null,"SY",null,null,0,null,0,null,4.5425E-2,null,2.2294719999999999]
[null,"0285-737","Optional Base (18\" Graded Aggregate) Project 410981-8-52-01",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-738","Optional Base (18\" Graded Aggregate) Project 431883-6-52-01",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-739","Optional Base (18\" Graded Aggregate) Project 439892-1-52-01",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-740","Optional Base (18\" Graded Aggregate) Project 217910-4-32-01",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-741","Optional Base (18\" Graded Aggregate) Project 443503-1-52-01",null,"SY",null,null,0,null,0,null,3.4069000000000002E-2,null,1.6733020000000001]
[null,"0285-742","Optional Base (21\" Graded Aggregate) Project 218594-2-52-01",null,"SY",null,null,0,null,0,null,4.1346000000000001E-2,null,1.920142]
[null,"0285-743","Optional Base (20\" Graded Aggregate) Project 442914-1-52-01",null,"SY",null,null,0,null,0,null,4.1346000000000001E-2,null,1.920142]
[null,"0285-744","Optional Base (15\" Graded Aggregate) Project 436273-1-52-01",null,"SY",null,null,0,null,0,null,3.2024999999999998E-2,null,1.518281]
[null,"0285-745","Optional Base (20\" Graded Aggregate) Project 421878-3-52-01",null,"SY",null,null,0,null,0,null,4.1346000000000001E-2,null,1.920142]
[null,"0285-746","Optional Base (4\" Graded Aggregate) Project 439457-1-52-01",null,"SY",null,null,0,null,0,null,1.9779000000000001E-2,null,0.58952599999999999]
[null,"0286-1","Turnout Construction",null,"SY",null,321321,0,null,0,null,7.3467000000000005E-2,null,0.51755300000000004]
[null,"0286-2","Turnout Construction",null,"TN",null,321321,0,null,0,null,4.0854000000000001E-2,null,1.6003369999999999]
[null,"0287-1","Permeable Base (Asphalt Treated) added 9/1/09",null,"CY",null,321321,{"$f":"ROUND(F73*L73,0)","v":0},null,{"$f":"ROUND(F73*N73,0)","v":0},null,8.7900000000000006E-2,null,1.5212000000000001]
[null,"0324-1","Rework Asphalt Concrete",null,"SY",null,null,{"$f":"ROUND(F74*L74,0)","v":0},null,{"$f":"ROUND(F74*N74,0)","v":0},null,9.7000000000000003E-3,null,3.1600000000000003E-2]
[null,"0327-70-1 ","Milling Existing Asph Pavmt. (1\" Avg. Depth)",null,"SY",null,321321,{"$f":"ROUND(F75*L75,0)","v":0},null,{"$f":"ROUND(F75*N75,0)","v":0},null,4.9600000000000002E-4,null,6.3597000000000001E-2]
[null,"0327-70-2","Milling Existing Asph Pavmt. (3 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.047E-3,null,0.13425999999999999]
[null,"0327-70-3","Milling Existing Asph Pavmt. (4 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.346E-3,null,0.17262]
[null,"0327-70-4","Milling Existing Asph Pavmt. (3\" Avg. Depth)",null,"SY",null,null,0,null,0,null,8.5599999999999999E-4,null,0.109849]
[null,"0327-70-5","Milling Existing Asph Pavmt. (2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,6.2799999999999998E-4,null,8.0556000000000003E-2]
[null,"0327-70-6","Milling Existing Asph Pavmt. (1 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,5.5400000000000002E-4,null,7.1079000000000003E-2]
[null,"0327-70-7","Milling Existing Asph Pavmt. (4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.256E-3,null,0.16111200000000001]
[null,"0327-70-8","Milling Existing Asph Pavmt. (2 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,7.2499999999999995E-4,null,9.2949000000000004E-2]
[null,"0327-70-9","Milling Existing Asph Pavmt. (5 1/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.5070000000000001E-3,null,0.19333400000000001]
[null,"0327-70-10","Milling Existing Asph Pavmt. (5\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.449E-3,null,0.18589800000000001]
[null,"0327-70-11","Milling Existing Asph Pavmt. (2 1/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,6.7299999999999999E-4,null,8.6309999999999998E-2]
[null,"0327-70-12","Milling Existing Asph Pavmt. (1 1/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,5.2300000000000003E-4,null,6.7129999999999995E-2]
[null,"0327-70-13","Milling Existing Asph Pavmt. (1 3/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,5.8900000000000001E-4,null,7.5521000000000005E-2]
[null,"0327-70-14","Milling Existing Asph Pavmt. (6 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-15","Milling Existing Asph Pavmt. (2 3/4\"\" Avg. Depth)",null,"SY",null,null,0,null,0,null,7.85E-4,null,0.10069500000000001]
[null,"0327-70-16","Milling Existing Asph Pavmt. (1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,4.4900000000000002E-4,null,5.7540000000000001E-2]
[null,"0327-70-17","Milling Existing Asph Pavmt. (3 1/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,9.4200000000000002E-4,null,0.120834]
[null,"0327-70-18","Milling Existing Asph Pavmt. (5 1/2\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.5699999999999999E-4,null,2.0035000000000001E-2]
[null,"0327-70-19","Milling Existing Asph Pavmt. (3/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,4.7100000000000001E-4,null,6.0416999999999998E-2]
[null,"0327-70-20","Milling Existing Asph Pavmt. (3 3/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.178E-3,null,0.15104300000000001]
[null,"0327-70-22","Milling Existing Asph Pavmt. (4 1/4\" Avg. Depth)",null,"SY",null,null,0,null,0,null,1.299E-3,null,0.16666800000000001]
[null,"0327-70-23","Mill Existing Asphalt Pavement (6\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-24","Mill Existing Asphalt Pavement (9\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-25","Mill Existing Asphalt Pavement (8\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-26","Mill Existing Asphalt Pavement (4 3/4\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-27","Mill Existing Asphalt Pavement (5 3/4\"Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-28","Mill Existing Asphalt Pavement (6 3/4\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-29","Mill Existing Asphalt Pavement (6 1/4\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-30","Mill Existing Asphalt Pavement (11 1/2\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-31","Mill Existing Asphalt Pavement (7 1/2\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-32","Mill Existing Asphalt Pavement (8 1/2\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-33","Mill Existing Asphalt Pavement (7 3/4\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-34","Mill Existing Asphalt Pavement (8\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F107*L107,0)","v":0},null,{"$f":"ROUND(F107*N107,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-35","Mill Existing Asphalt Pavement (8 1/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F108*L108,0)","v":0},null,{"$f":"ROUND(F108*N108,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-36","Mill Existing Asphalt Pavement (9 1/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F109*L109,0)","v":0},null,{"$f":"ROUND(F109*N109,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-37","Mill Existing Asphalt Pavement (9 1/2\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F110*L110,0)","v":0},null,{"$f":"ROUND(F110*N110,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-38","Mill Existing Asphalt Pavement (8 3/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F111*L111,0)","v":0},null,{"$f":"ROUND(F111*N111,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-39","Mill Existing Asphalt Pavement (9\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F112*L112,0)","v":0},null,{"$f":"ROUND(F112*N112,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-40","Mill Existing Asphalt Pavement (10\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F113*L113,0)","v":0},null,{"$f":"ROUND(F113*N113,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-41","Mill Existing Asphalt Pavement (10 1/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F114*L114,0)","v":0},null,{"$f":"ROUND(F114*N114,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-42","Mill Existing Asphalt Pavement (7 1/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F115*L115,0)","v":0},null,{"$f":"ROUND(F115*N115,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-44","Mill Existing Asphalt Pavement (12 1/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F116*L116,0)","v":0},null,{"$f":"ROUND(F116*N116,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-45","Mill Existing Asphalt Pavement (12 3/4\" Avg Depth)",null,"SY",null,null,{"$f":"ROUND(F117*L117,0)","v":0},null,{"$f":"ROUND(F117*N117,0)","v":0},null,1.7129999999999999E-3,null,0.219698]
[null,"0327-70-46","Mill Existing Asphalt Pavement (12\" Avg Depth)",null,"SY",null,null,0,null,0,null,1.7129999999999999E-3,null,0.219698]
[null,"0334-1-11","Superpave Asphalt Concrete (Traffic Level A)",null,"TN",null,321321,{"$f":"ROUND(F119*L119,0)","v":0},null,{"$f":"ROUND(F119*N119,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-12","Superpave Asphalt Concrete (Traffic Level B)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-13","Superpave Asphalt Concrete (Traffic Level C)",null,"TN",null,null,{"$f":"ROUND(F121*L121,0)","v":0},null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-14","Superpave Asphalt Concrete (Traffic Level D)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-15","Superpave Asphalt Concrete (Traffic Level E)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-22","Superpave Asphalt Concrete (Traffic B) PG76-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-23","Superpave Asphalt Concrete (Traffic C) PG76-22 PMA",null,"TN",null,null,{"$f":"ROUND(F125*L125,0)","v":0},null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-24","Superpave Asphalt Concrete (Traffic D) PG76-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-25","Superpave Asphalt Concrete (Traffic E) PG76-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-33","Superpave Asphalt Concrete (Traffic C) PG82-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-34","Superpave Asphalt Concrete (Traffic D) PG82-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-35","Superpave Asphalt Concrete (Traffic E) PG82-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-43","Superpave Asphalt Concrete (Traffic C) PG76-22 ",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-52","Superpave Asphalt Concrete (Traffic B) PG76-22 ",null,"TN",null,null,{"$f":"ROUND(F132*L132,0)","v":0},null,{"$f":"ROUND(F132*N132,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-53","Superpave Asphalt Concrete (Traffic C) PG76-22 ",null,"TN",null,null,{"$f":"ROUND(F133*L133,0)","v":0},null,{"$f":"ROUND(F133*N133,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-54","Superpave Asphalt Concrete (Traffic D) PG76-22 ",null,"TN",null,null,{"$f":"ROUND(F134*L134,0)","v":0},null,{"$f":"ROUND(F134*N134,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-55","Superpave Asphalt Concrete (Traffic E) PG76-22 ",null,"TN",null,null,{"$f":"ROUND(F135*L135,0)","v":0},null,{"$f":"ROUND(F135*N135,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-56","Superpave Asphalt Concrete (Traffic B) High Polymer",null,"TN",null,null,{"$f":"ROUND(F136*L136,0)","v":0},null,{"$f":"ROUND(F136*N136,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-57","Superpave Asphalt Concrete (Traffic C) High Polymer",null,"TN",null,null,{"$f":"ROUND(F137*L137,0)","v":0},null,{"$f":"ROUND(F137*N137,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-58","Superpave Asphalt Concrete (Traffic D) High Polymer",null,"TN",null,null,{"$f":"ROUND(F138*L138,0)","v":0},null,{"$f":"ROUND(F138*N138,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0334-1-59","Superpave Asphalt Concrete (Traffic E) High Polymer",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-5","Asphalt Concrete Friction Course (FC5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-6","Asphalt Concrete Friction Course (FC12.5) (FC 6)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-7","Asphalt Concrete Friction Course (FC9.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-20","Asp Conc.Friction Course (FC12.5)(FC 6) PG76-22",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-21","Asp Conc.Friction Course (FC9.5) PG76-22",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-22","Asp Conc.Friction Course (FC 5) PG76-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-23","Asp Conc.Friction Course, Incl. Bit,(FC5) PG82-22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-24","Asp Conc.Friction Course (FC5) PG76-22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-25","Asp Conc.Friction Course Incl. Bit, (FC5) PG 76-22",null,"TN",null,null,{"$f":"ROUND(F148*L148,0)","v":0},null,{"$f":"ROUND(F148*N148,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-26","Asp Conc.Friction Course Incl. Bit, (FC5) PG 76-22 High Polymer",null,"TN",null,null,{"$f":"ROUND(F149*L149,0)","v":0},null,{"$f":"ROUND(F149*N149,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-29","Asp Conc.Friction Course (Traffic B)(FC4.75) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-30","Asp Conc.Friction Course (Traffic B)(FC9.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-31","Asp Conc.Friction Course (Traffic B)(FC12.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-32","Asp Conc.Friction Course (Traffic C)(FC9.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-33","Asp Conc.Friction Course (Traffic C)(FC12.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-35","Asp Conc.Friction Course (Traffic D)(FC12.5) (Rubber)",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-39","Asp Conc.Fric Course (Traffic B)(FC4.75) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-40","Asp Conc.Fric Course (Traffic B)(FC9.5) PG76.22 PMA ",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-41","Asp Conc.Fric Course (Traffic B)(FC12.5) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-42","Asp Conc.Fric Course (Traffic C)(FC9.5) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-43","Asp Conc.Fric Course (Traffic C)(FC12.5) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-45","Asp Conc.Fric Course (Traffic D)(FC12.5) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-48","Asp Conc.Fric Course (Traffic E)(FC12.5) PG76.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-54","Asp Conc.Fric Course (Traffic C)(FC9.5) PG82.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-55","Asp Conc.Fric Course (Traffic C)(FC12.5) PG82.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-58","Asp Conc.Fric Course (Traffic D)(FC12.5) PG82.22 PMA",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-70","Asp Conc.Fric Course (Traffic B)(FC4.75) PG76.22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-71","Asp Conc.Fric Course (Traffic B)(FC9.5) PG76.22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-72","Asp Conc.Fric Course (Traffic B)(FC12.5) PG76.22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-73","Asp Conc.Fric Course (Traffic C)(FC9.5) PG76.22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-74","Asp Conc.Fric Course (Traffic C)(FC12.5) PG76.22 ARB",null,"TN",null,null,0,null,0,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-80","Asp Conc.Fric Course (Traffic B)(FC9.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F171*L171,0)","v":0},null,{"$f":"ROUND(F171*N171,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-81","Asp Conc.Fric Course (Traffic B)(FC12.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F172*L172,0)","v":0},null,{"$f":"ROUND(F172*N172,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-82","Asp Conc.Fric Course (Traffic C)(FC9.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F173*L173,0)","v":0},null,{"$f":"ROUND(F173*N173,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-83","Asp Conc.Fric Course (Traffic C)(FC12.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F174*L174,0)","v":0},null,{"$f":"ROUND(F174*N174,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-85","Asp Conc.Fric Course (Traffic D)(FC12.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F175*L175,0)","v":0},null,{"$f":"ROUND(F175*N175,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-88","Asp Conc.Fric Course (Traffic E)(FC12.5) PG76.22",null,"TN",null,null,{"$f":"ROUND(F176*L176,0)","v":0},null,{"$f":"ROUND(F176*N176,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-90","Asp Conc.Fric Course (Traffic B)(FC9.5), High Polymer",null,"TN",null,null,{"$f":"ROUND(F177*L177,0)","v":0},null,{"$f":"ROUND(F177*N177,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-91","Asp Conc.Fric Course (Traffic B)(FC12.5), High Polymer",null,"TN",null,null,null,null,null,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-92","Asp Conc.Fric Course (Traffic C)(FC9.5), High Polymer",null,"TN",null,null,null,null,null,null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-93","Asp Conc.Fric Course (Traffic C)(FC12.5), High Polymer",null,"TN",null,null,{"$f":"ROUND(F180*L180,0)","v":0},null,{"$f":"ROUND(F180*N180,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0337-7-94","Asp Conc.Fric Course (Traffic D)(FC12.5), High Polymer",null,"TN",null,null,{"$f":"ROUND(F181*L181,0)","v":0},null,{"$f":"ROUND(F181*N181,0)","v":0},null,6.1899999999999997E-2,null,3.281625]
[null,"0339-1","Miscellaneous Asphalt Pavement",null,"TN",null,321321,0,null,0,null,0.12379999999999999,null,3.1603729999999999]
[null,"0350-1-1","Plain Cement Concrete Pavmt. 6\"",null,"SY",null,321321,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-2","Plain Cement Concrete Pavmt. 7\"",null,"SY",null,null,{"$f":"ROUND(F184*L184,0)","v":0},null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-3","Plain Cement Concrete Pavmt. 8\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-4","Plain Cement Concrete Pavmt. 9\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-5","Plain Cement Concrete Pavmt. 10\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-8","Plain Cement Concrete Pavmt. Plain. 7 1/2 \"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-10","Plain Cement Concrete Pavmt. 12\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-11","Plain Cement Concrete Pavmt. 13\"",null,"SY",null,null,0,null,0,null,0.18316099999999999,null,0.11969399999999999]
[null,"0350-1-12","Plain Cement Concrete Pavmt. 11\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-13","Plain Cement Concrete Pavmt. 11 1/2\"",null,"SY",null,null,0,null,0,null,0.1792,null,0.11082699999999999]
[null,"0350-1-14","Plain Cement Concrete Pavmt. 14\"",null,"SY",null,null,0,null,0,null,0.18449099999999999,null,0.12267]
[null,"0350-1-15","Plain Cement Concrete Pavmt. 13 1/2\"",null,"SY",null,null,0,null,0,null,0.18316099999999999,null,0.11969399999999999]
[null,"0350-1-16","Plain Cement Concrete Pavmt. 10 1/2\"",null,"SY",null,null,0,null,0,null,0.1792,null,0.11082699999999999]
[null,"0350-1-19","Plain Cement Concrete Pavmt. 12 1/2\"",null,"SY",null,null,0,null,0,null,0.1792,null,0.11082699999999999]
[null,"0350-1-20","Plain Cement Concrete Pavmt. Var. 9 1/2\" Avg.",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-1-21","Plain Cement Concrete Pavmt. Var. 11\" Avg.",null,"SY",null,null,0,null,0,null,0.1792,null,0.11082699999999999]
[null,"0350-1-22","Plain Cement Concrete Pavmt. Var. 11 1/2\" Avg.",null,"SY",null,null,0,null,0,null,0.1792,null,0.11082699999999999]
[null,"0350-1-23","Plain Cement Concrete Pavmt. 14 1/2\"",null,"SY",null,null,0,null,0,null,0.185807,null,0.125615]
[null,"0350-2-1 ","Cement Concrete Pavmt. Reinforced 6\" ",null,"SY",null,null,{"$f":"ROUND(F201*L201,0)","v":0},null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-2-3","Cement Concrete Pavmt. Reinforced 8\" ",null,"SY",null,null,0,null,0,null,0.17918600000000001,0.17918600000000001,0.110795]
[null,"0350-2-4","Cement Concrete Pavmt. Reinforced 9\" ",null,"SY",null,null,0,null,0,null,0.17918600000000001,0.17918600000000001,0.110795]
[null,"0350-2-10","Cement Concrete Pavmt. Reinforced 12\" ",null,"SY",null,null,0,null,0,null,0.17918600000000001,0.17918600000000001,0.110795]
[null,"0350-2-12","Cement Concrete Pavmt. Reinforced 11\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,0.17918600000000001,0.110795]
[null,"0350-2-17","Cement Concrete Pavmt. Reinforced 8.5\" ",null,"SY",null,null,0,null,0,null,0.17918600000000001,0.17918600000000001,0.110795]
[null,"0350-3-6","Plain Cement Concrete Pavmt. 8.5\"",null,"SY",null,null,0,null,0,null,0.17918600000000001,null,0.110795]
[null,"0350-3-14","Cement Concrete Pavmt. 12.5\" ",null,"SY",null,null,{"$f":"ROUND(F208*L208,0)","v":0},null,{"$f":"ROUND(F208*N208,0)","v":0},null,0.18449099999999999,null,0.12267]
[null,"0350-3-15","Cement Concrete Pavmt. 13\" ",null,"SY",null,null,null,null,null,null,0.18449099999999999,null,0.12267]
[null,"0350-3-17","Cement Concrete Pavmt. Reinforced 14\" ",null,"SY",null,null,0,null,0,null,0.18449099999999999,null,0.12267]
[null,"0350-3-18","Cement Concrete Pavmt. Reinforced 14.5\" ",null,"SY",null,null,0,null,0,null,0.18449099999999999,null,0.12267]
[null,"0350-4-11","Cement Concrete Pavmt. Reinforced 11\" ",null,"SY",null,null,{"$f":"ROUND(F212*L212,0)","v":0},null,{"$f":"ROUND(F212*N212,0)","v":0},null,0.17918600000000001,null,0.110795]
[null,"0350-30-5","Concrete Pavmt. for Roundabout Apron, 8\" Depth",null,"SY",null,null,0,null,0,null,0.18449099999999999,null,0.12267]
[null,"0350-30-13","Concrete Pavmt. for Roundabout Apron, 12\" Depth",null,"SY",null,null,{"$f":"ROUND(F214*L214,0)","v":0},null,{"$f":"ROUND(F214*N214,0)","v":0},null,0.18449099999999999,null,0.12267]
[null,"0400-0-11 ","Concrete Class NS, Gravity Wall ",null,"CY",null,null,0,null,0,null,9.1306119999999993,null,4.1204080000000003]
[null,"0400-0-13","Concrete Class NS, Steps",null,"CY",null,null,{"$f":"ROUND(F216*L216,0)","v":0},null,0,null,9.1306119999999993,null,4.1204080000000003]
[null,"0400-1-1","Concrete Class I, Culverts",null,"CY",null,null,0,null,0,null,9.3800000000000008,null,13.514469]
[null,"0400-1-2","Concrete Class I, Endwalls",null,"CY",null,null,0,null,0,null,9.1306119999999993,null,4.1204080000000003]
[null,"0400-1-5","Concrete Class I, Substructure",null,"CY",null,null,0,null,0,null,6.3914289999999996,null,11.18]
[null,"0400-1-11","Concrete Class I, Retaininh Walls",null,"CY",null,null,0,null,0,null,5.9653330000000002,null,2.9493330000000002]
[null,"0400-1-15","Concrete Class I, Miscelaneous",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-1-25","Concrete Class I, Mass Substructure",null,"CY",null,null,0,null,0,null,7.0035150000000002,null,3.219684]
[null,"0400-2-1","Concrete Class II, Culverts",null,"CY",null,null,0,null,0,null,9.3810640000000003,null,13.514469]
[null,"0400-2-2","Concrete Class II, Endwalls",null,"CY",null,null,0,null,0,null,9.1306119999999993,null,4.1204080000000003]
[null,"0400-2-4","Concrete Class II, Superstructure",null,"CY",null,null,0,null,0,null,7.9566790000000003,null,6.1991509999999996]
[null,"0400-2-5","Concrete Class II, Substructure",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-2-8","Concrete Class II, Bulkead",null,"CY",null,null,0,null,0,null,6.6478450000000002,null,1.653789]
[null,"0400-2-10","Concrete Class II, Approach Slabs",null,"CY",null,null,0,null,0,null,2.346174,null,0.45593699999999998]
[null,"0400-2-11","Concrete Class II, Retaining Walls",null,"CY",null,null,0,null,0,null,5.9653330000000002,null,2.9493330000000002]
[null,"0400-2-12","Concrete Class II, Trenc Slab",null,"CY",null,null,0,null,0,null,3.213803,null,1.153788]
[null,"0400-2-15","Concrete Class II, Miscelaneous",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-2-25","Concrete Class II, Mass Substructure",null,"CY",null,null,0,null,0,null,6.3381670000000003,null,10.444667000000001]
[null,"044-2-41","Concrete Class II, Precast Deck Overlay",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-3-1","Concrete Class III, Culverts",null,"CY",null,null,0,null,0,null,9.3810640000000003,null,13.514469]
[null,"0400-3-8","Concrete Class III, Bulkhead",null,"CY",null,null,0,null,0,null,6.6478450000000002,null,1.653789]
[null,"0400-3-15","Concrete Class III, Miscellaneous",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-3-20","Concrete Class III, Seal",null,"CY",null,null,0,null,0,null,0.95018800000000003,null,3.7000459999999999]
[null,"0400-3-45","Concrete Class III, Precast Substructure",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-4-1","Concrete Class IV, Cuverts",null,"CY",null,null,0,null,0,null,9.3810640000000003,null,13.514469]
[null,"0400-4-2","Concrete Class IV, Endwalls",null,"CY",null,null,0,null,0,null,9.1306119999999993,null,4.1204080000000003]
[null,"0400-4-4","Concrete Class IV, Superstructure",null,"CY",null,null,0,null,0,null,7.9566790000000003,null,6.1991509999999996]
[null,"0400-4-5","Concrete Class IV, Substructure",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-4-6","Concrete Class IV, Counterweight",null,"CY",null,null,0,null,0,null,9.2850000000000001,null,3.410196]
[null,"0400-4-8","Concrete Class IV, Bulkhead",null,"CY",null,null,0,null,0,null,6.6478450000000002,null,1.8573550000000001]
[null,"0400-4-11","Concrete Class IV, Retaining Walls",null,"CY",null,null,0,null,0,null,5.9653330000000002,null,2.9493330000000002]
[null,"0400-4-15","Concrete Class IV, Miscellaneous",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-4-22","Concrete Class IV, Superstructure Closure Joint",null,"CY",null,null,0,null,0,null,4.1181429999999999,null,0.607595]
[null,"0400-4-25","Concrete Class IV, Mass Substructure",null,"CY",null,null,0,null,0,null,6.3381670000000003,null,11.260667]
[null,"0400-4-39","Concrete Class IV, Precast Seg. Superstructure",null,"CY",null,null,0,null,0,null,2.7207170000000001,null,24.523427999999999]
[null,"0400-4-40","Concrete Class IV, Precast Seg. Substructure",null,"CY",null,null,0,null,0,null,2.7207170000000001,null,24.523427999999999]
[null,"0400-4-41","Concrete Class IV, Precast Deck Overlay",null,"CY",null,null,0,null,0,null,4.4740000000000002,null,1.538]
[null,"0400-4-47","Concrete Class IV, CIP Topping with Shrinkage Reducing Admix",null,"CY",null,null,{"$f":"ROUND(F252*L252,0)","v":0},null,{"$f":"ROUND(F252*N252,0)","v":0},null,4.4740000000000002,null,1.538]
[null,"0400-4-104","Concrete Class IV, Superstructure. LT-WT",null,"CY",null,null,{"$f":"ROUND(F253*L253,0)","v":0},null,0,null,7.9566790000000003,null,6.1991509999999996]
[null,"0400-8-4","Concrete Class V, Superstructure",null,"CY",null,null,{"$f":"ROUND(F254*L254,0)","v":0},null,{"$f":"ROUND(F254*N254,0)","v":0},null,7.9566790000000003,null,6.1991509999999996]
[null,"0400-8-5","Concrete Class V, Substructure",null,"CY",null,321321,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-8-22","Concrete Class V, Superstructure Closeout Joint",null,"CY",null,null,0,null,0,null,4.1181429999999999,null,0.607595]
[null,"0400-8-25","Concrete Class V, Mass Substructure",null,"CY",null,null,0,null,0,null,6.3381670000000003,null,11.260667]
[null,"0400-8-39","Concrete Class V, Precast Seg. Superstructure",null,"CY",null,null,0,null,0,null,2.7207170000000001,null,23.987043]
[null,"0400-8-105","Concrete Class V, Substructure Special",null,"CY",null,null,0,null,0,null,7.9566790000000003,null,6.1991509999999996]
[null,"0400-8-106","Concrete Class V, Microsilica Substructure",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-8-107","Concrete Class V, Microsilica Substructure Mass",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-16-22","Concrete Class VI, Superstructure Closure Joint",null,"CY",null,321321,0,null,0,null,4.1181429999999999,null,0.607595]
[null,"0400-16-25","Concrete Class VI, Mass Substructure ",null,"CY",null,null,0,null,0,null,6.3381670000000003,null,11.260667]
[null,"0400-16-39","Concrete Class VI, Precast Seg. Superstructure ",null,"CY",null,null,0,null,0,null,2.7207170000000001,null,24.523427999999999]
[null,"0400-16-42","Concrete Class VI, Substructure Self-Consolidating",null,"CY",null,null,0,null,0,null,11.736793,null,4.8538899999999998]
[null,"0400-16-43","Concrete Class VI, Superstructure Self-Consolidating",null,"CY",null,null,0,null,0,null,7.9566790000000003,null,6.1991509999999996]
[null,"0407-1-11","Precast Concrete 3 Side Box Culvert 0-19' Span, < or = 10' Height",null,"LF",null,null,0,null,0,null,3.3508049999999998,null,7.14825]
[null,"0407-1-21","Precast Concrete 3 Side Box Culvert 20-29' Span, < or = 10' Height",null,"LF",null,null,0,null,0,null,3.3508049999999998,null,7.14825]
[null,"0407-1-52","Precast Concrete 3 Side Box Culvert 50' Span or >, 10' Height or >",null,"LF",null,321321,{"$f":"ROUND(F269*L269,0)","v":0},null,{"$f":"ROUND(F269*N269,0)","v":0},null,3.3508049999999998,null,7.14825]
[null,"0410-70-84","PCBC, F & I, 8 Span, 4 Ht",null,"LF",null,321321,0,null,0,null,3.3508049999999998,null,7.14825]
[null,"0410-7100","PCBC, F & I, 10 Span, 10 or > Ht",null,"LF",null,null,0,null,0,null,4.350848,null,11.222148000000001]
[null,"0410-7104","PCBC, F & I, 10 Span, 4 Ht",null,"LF",null,null,0,null,0,null,3.3508049999999998,null,7.14825]
[null,"0415-1-1","Reinforcing Steel- Roadway",null,"LB",null,321321,0,null,0,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-1- 2","Reinforcing Steel- Bridge",null,"LB",null,null,0,null,0,null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-3","Reinforcing Steel- Retaining Wall",null,"LB",null,null,0,null,0,null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-4","Reinforcing Steel- Super Structure",null,"LB",null,null,{"$f":"ROUND(F276*L276,0)","v":0},null,0,null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-5","Reinforcing Steel- Substructure",null,"LB",null,null,0,null,0,null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-6","Reinforcing Steel- Miscellaneous",null,"LB",null,null,0,null,0,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-1-7","Reinforcing Steel- Sound Barrier Wall",null,"LB",null,null,0,null,{"$f":"ROUND(F279*N279,0)","v":0},null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-8","Reinforcing Steel- Bulkhead",null,"LB",null,null,0,null,{"$f":"ROUND(F280*N280,0)","v":0},null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-1-9","Reinforcing Steel- Approach Slabs",null,"LB",null,null,0,null,0,null,1.769E-3,null,8.1999999999999998E-4]
[null,"0415-1-13","Reinforcing Steel- Steps",null,"LB",null,null,0,null,0,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-2-4","Reinforcing Steel- Stainless, Superstructure",null,"LB",null,null,null,null,null,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-2-5","Reinforcing Steel- Stainless, Substructure",null,"LB",null,null,null,null,null,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-2-6","Reinforcing Steel- Stainless, Miscellaneous",null,"LB",null,null,{"$f":"ROUND(F285*L285,0)","v":0},null,0,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-2-8","Reinforcing Steel- Stainless, Bulkhhead",null,"LB",null,null,0,null,0,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0415-2-9","Reinforcing Steel- Stainless, Approach Slabs",null,"LB",null,null,null,null,null,null,2.9710000000000001E-3,null,9.19E-4]
[null,"0425-1201","Inlets, Curb. Type 9,<10",null,"EA",null,null,0,null,0,null,30.883334000000001,null,40.950000000000003]
[null,"0425-1202","Inlets, Curb. Type 9,>10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1203","Inlets, Curb. Type 9, J Bottom <10",null,"EA",null,null,0,null,0,null,61.766666000000001,null,81.900000000000006]
[null,"0425-1205","Inlets, Curb. Type 9, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1209","Inlets, Curb. Type 9, Modify",null,"EA",null,null,0,null,0,null,32.183334000000002,null,40.950000000000003]
[null,"0425-1211","Inlets, Curb. Type 10,<10",null,"EA",null,null,0,null,0,null,30.883334000000001,null,40.950000000000003]
[null,"0425-1213","Inlets, Curb. Type 10, J Bottom <10",null,"EA",null,null,0,null,0,null,30.883334000000001,null,40.950000000000003]
[null,"0425-1215","Inlets, Curb. Type 10, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1311","Inlets, Curb. Type P-1,<10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1312","Inlets, Curb. Type P-1,>10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1315","Inlets, Curb. Type P-1, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1319","Inlets, Curb. Type P-1, Modify",null,"EA",null,null,0,null,0,null,32.183334000000002,null,40.950000000000003]
[null,"0425-1321","Inlets, Curb. Type P-2,<10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1322","Inlets, Curb. Type P-2,>10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1325","Inlets, Curb. Type P-2, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1329","Inlets, Curb. Type P-2, Modify",null,"EA",null,null,0,null,0,null,32.183334000000002,null,40.950000000000003]
[null,"0425-1331","Inlets, Curb. Type P-3, <10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1332","Inlets, Curb. Type P-3, >10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1335","Inlets, Curb. Type P-3, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1341","Inlets, Curb. Type P-4, <10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1342","Inlets, Curb. Type P-4, >10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1345","Inlets, Curb. Type P-4, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1349","Inlets, Curb. Type P-4, Modify",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1351","Inlets, Curb. Type P-5, <10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1352","Inlets, Curb. Type P-5, >10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1355","Inlets, Curb. Type P-5, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1359","Inlets, Curb. Type P-5, Modify",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1361","Inlets, Curb. Type P-6, <10",null,"EA",null,null,0,null,0,null,33.602021000000001,null,40.950000000000003]
[null,"0425-1362","Inlets, Curb. Type P-6, >10",null,"EA",null,null,0,null,0,null,43.981414000000001,null,49.636364]
[null,"0425-1365","Inlets, Curb. Type P-6, Partial",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1369","Inlets, Curb. Type P-6, Modify",null,"EA",null,null,0,null,0,null,29.988686999999999,null,32.76]
[null,"0425-1411","Inlets, Curb. Type J-1, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1412","Inlets, Curb. Type J-1, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1415","Inlets, Curb. Type J-1, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1419","Inlets, Curb. Type J-1, Modify",null,"EA",null,null,0,null,0,null,32.183334000000002,null,65.400000000000006]
[null,"0425-1421","Inlets, Curb. Type J-2, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1422","Inlets, Curb. Type J-2, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1425","Inlets, Curb. Type J-2, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1429","Inlets, Curb. Type J-2, Modify",null,"EA",null,null,0,null,0,null,32.183346999999998,null,40.950000000000003]
[null,"0425-1431","Inlets, Curb. Type J-3, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1432","Inlets, Curb. Type J-3, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1435","Inlets, Curb. Type J-3, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1441","Inlets, Curb. Type J-4, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1442","Inlets, Curb. Type J-4, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1445","Inlets, Curb. Type J-4, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1451","Inlets, Curb. Type J-5, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1452","Inlets, Curb. Type J-5, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1455","Inlets, Curb. Type J-5, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1459","Inlets, Curb. Type J-5, Modify",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1461","Inlets, Curb. Type J-6, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1462","Inlets, Curb. Type J-6, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1465","Inlets, Curb. Type J-6, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1471","Inlets, Curb. Type J-7, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1472","Inlets, Curb. Type J-7, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1473","Inlets, Curb. Type J-7, J Bottom, <10",null,"EA",null,null,0,null,0,null,39.624243,null,87.2]
[null,"0425-1474","Inlets, Curb. Type J-7, J Bottom, >10",null,"EA",null,null,0,null,0,null,46.328888999999997,null,87.2]
[null,"0425-1475","Inlets, Curb. Type J-7, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1479","Inlets, Curb. Type J-7, Modify",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1481","Inlets, Curb. Type J-8, <10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1482","Inlets, Curb, Type 8, >10",null,"EA",null,null,0,null,0,null,36.182972999999997,null,74.742857000000001]
[null,"0425-1483","Inlets, Curb. Type J-8, J Bottom, <10",null,"EA",null,null,0,null,0,null,39.624243,null,87.2]
[null,"0425-1484","Inlets, Curb. Type J-8, J Bottom, >10",null,"EA",null,null,0,null,{"$f":"ROUND(F349*N349,0)","v":0},null,46.328888999999997,null,87.2]
[null,"0425-1485","Inlets, Curb. Type J-8, Partial",null,"EA",null,null,0,null,0,null,31.594612999999999,null,58.133333]
[null,"0425-1489","Inlets, Curb. Type J-8, Modify",null,"EA",null,null,0,null,0,null,32.183334000000002,null,65.400000000000006]
[null,"0425-1501","Inlets, Ditch Bot. Type A, <10",null,"EA",null,null,0,null,0,null,21.956363,null,39.905455000000003]
[null,"0425-1502","Inlets, Ditch Bot. Type A, >10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1503","Inlets, Ditch Bot. Type A, J Bottom, <10",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1504","Inlets, Ditch Bot. Type A, J Bottom, >10",null,"EA",null,null,0,null,0,null,28.537037000000002,null,74.133332999999993]
[null,"0425-1505","Inlets, Ditch Bot. Type A, Partial",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1511","Inlets, Ditch Bot. Type B, <10",null,"EA",null,null,0,null,0,null,21.956363,null,39.905455000000003]
[null,"0425-1512","Inlets, Ditch Bot. Type B, >10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1513","Inlets, Ditch Bot. Type B, J Bottom, <10",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1514","Inlets, Ditch Bot. Type B, J Bottom, >10",null,"EA",null,null,0,null,0,null,28.537037000000002,null,74.133332999999993]
[null,"0425-1515","Inlets, Ditch Bot. Type B, Partial",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1519","Inlets, Ditch Bot. Type B Modify",null,"EA",null,null,0,null,0,null,22.996362999999999,null,39.905455000000003]
[null,"0425-1521","Inlets, Ditch Bot. Type C, < 10 ",null,"EA",null,null,0,null,0,null,21.956363,null,39.905455000000003]
[null,"0425-1522","Inlets, Ditch Bot. Type C, >10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1523","Inlets, Ditch Bot. Type C, J Bottom, <10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1524","Inlets, Ditch Bot. Type C, J Bottom, >10",null,"EA",null,null,0,null,0,null,28.537037000000002,null,74.133332999999993]
[null,"0425-1525","Inlets, Ditch Bot. Type C, Partial",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1529","Inlets, Ditch Bot. Type C, Modify",null,"EA",null,null,0,null,0,null,22.996362999999999,null,39.905455000000003]
[null,"0425-1531","Inlets, Ditch Bot. Type C, Modify, <10",null,"EA",null,null,0,null,0,null,21.956363,null,39.905455000000003]
[null,"0425-1532","Inlets, Ditch Bot. Type C, Modify, >10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1533","Inlets, Ditch Bot. Type C, Modify, J Bottom, <10",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1534","Inlets, Ditch Bot. Type C, Modify, J Bottom, > 10",null,"EA",null,null,0,null,0,null,28.537037000000002,null,74.133332999999993]
[null,"0425-1535","Inlets, Ditch Bot. Type C, Modified, Partial",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1541","Inlets, Ditch Bot. Type D, <10",null,"EA",null,null,0,null,0,null,21.956363,null,39.905455000000003]
[null,"0425-1542","Inlets, Ditch Bot. Type D, >10",null,"EA",null,null,0,null,0,null,25.468147999999999,null,44.26]
[null,"0425-1543","Inlets, Ditch Bot. Type D, J Bottom, <10",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1544","Inlets, Ditch Bot. Type D, U Bottom, > 10 ",null,"EA",null,null,0,null,0,null,28.537037000000002,null,74.133332999999993]
[null,"0425-1545","Inlets, Ditch Bot. Type D, Partial ",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1547","Inlets, Ditch Bot. Type D, J Bottom, < 10, SPL ",null,"EA",null,null,0,null,0,null,24.312591999999999,null,44.26]
[null,"0425-1549","Inlets, Ditch Bot. Type D, Modify ",null,"EA",null,null,0,null,0,null,22.996362999999999,null,39.905455000000003]
[null,"0425-1551","Inlets, Ditch Bot. Type E, < 10 ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1552","Inlets, Ditch Bot. Type E, > 10 ",null,"EA",null,null,0,null,0,null,20.995555,null,38]
[null,"0425-1553","Inlets, Ditch Bot. Type E, J Bottom, < 10 ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1554","Inlets, Ditch Bot. Type E, J Bottom, > 10 ",null,"EA",null,null,0,null,0,null,20.995555,null,57.56]
[null,"0425-1555","Inlets, Ditch Bot. Type E, Partial ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1557","Inlets, Ditch Bot. Type E, J Bottom, < 10, SPL ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1559","Inlets, Ditch Bot. Type E, Modify ",null,"EA",null,null,0,null,0,null,20.995555,null,38]
[null,"0425-1561","Inlets, Ditch Bot. Type F, < 10 ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1562","Inlets, Ditch Bot. Type F, > 10 ",null,"EA",null,null,{"$f":"ROUND(F389*L389,0)","v":0},null,0,null,20.995555,null,38]
[null,"0425-1563","Inlets, Ditch Bot. Type F, J Bottom, < 10 ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1564","Inlets, Ditch Bot. Type F, J Bottom, > 10 ",null,"EA",null,null,0,null,0,null,20.995555,null,57.56]
[null,"0425-1565","Inlets, Ditch Bot. Type F, Partial ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1567","Inlets, Ditch Bot. Type F, J Bottom, < 10, SPL ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1568","Inlets, Ditch Bot. Type F, J Bottom, > 10, SPL ",null,"EA",null,null,0,null,0,null,20.995555,null,57.56]
[null,"0425-1569","Inlets, Ditch Bot. Type F, Modify ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1571","Inlets, Ditch Bot. Type G, < 10 ",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1572","Inlets, Ditch Bot. Type G, > 10 ",null,"EA",null,null,0,null,0,null,20.995555,null,40.619999999999997]
[null,"0425-1573","Inlets, Ditch Bot. Type G, J Bottom, < 10 ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1574","Inlets, Ditch Bot. Type G, J Bottom, > 10 ",null,"EA",null,null,0,null,0,null,20.995555,null,57.56]
[null,"0425-1575","Inlets, Ditch Bot. Type G, Partial ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1577","Inlets, Ditch Bot. Type G, J Bottom, < 10, SPL ",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1578","Inlets. Ditch Bot. Type G, J Bottom, > 10, SPL",null,"EA",null,null,0,null,0,null,20.995555,null,57.56]
[null,"0425-1579","Inlets. Ditch Bot. Type G, Modify",null,"EA",null,null,0,null,0,null,20.995555,null,38]
[null,"0425-1581","Inlets. Ditch Bot. Type H, < 10",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1582","Inlets. Ditch Bot. Type H, > 10",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1583","Inlets. Ditch Bot. Type H, J Bottom, < 10",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1584","Inlets. Ditch Bot. Type H, J Bottom, > 10",null,"EA",null,null,{"$f":"ROUND(F407*L407,0)","v":0},null,{"$f":"ROUND(F407*N407,0)","v":0},null,19.955555,null,38]
[null,"0425-1585","Inlets. Ditch Bot. Type H, Partial",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1587","Inlets. Ditch Bot. Type H, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1589","Inlets. Ditch Bot. Type H, Modify",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1601","Inlets. Ditch Bot. Type J, < 10",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1602","Inlets. Ditch Bot. Type J, > 10",null,"EA",null,null,0,null,0,null,20.995555,null,38]
[null,"0425-1603","Inlets. Ditch Bot. Type J, J Bottom, < 10",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1604","Inlets. Ditch Bot. Type J, J Bottom, > 10",null,"EA",null,null,0,null,{"$f":"ROUND(F414*N414,0)","v":0},null,20.995555,null,57.56]
[null,"0425-1605","Inlets. Ditch Bot. Type J, Partial",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1609","Inlets. Ditch Bot. Type J, Modify",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1611","Inlets. Ditch Bot. Type K, < 10",null,"EA",null,null,0,null,0,null,22.706665999999998,null,40.619999999999997]
[null,"0425-1617","Inlets. Ditch Bot. Type K, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,19.955555,null,38]
[null,"0425-1619","Inlets. Ditch Bot. Type K,  Bottom, Modify",null,"EA",null,null,0,null,0,null,23.746666000000001,null,40.619999999999997]
[null,"0425-1701","Inlets. Gutter, Type S, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1702","Inlets. Gutter, Type S, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1703","Inlets. Gutter, Type S, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1704","Inlets. Gutter, Type S, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1705","Inlets. Gutter, Type S, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1707","Inlets. Gutter, Type S, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1708","Inlets. Gutter, Type S, J Bottom, > 10, SPL",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1711","Inlets. Gutter, Type V, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1712","Inlets. Gutter, Type V, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1713","Inlets. Gutter, Type V, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1714","Inlets. Gutter Type V, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1715","Inlets. Gutter, Type V, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1719","Inlets. Gutter,Type V, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1725","Inlets. Gutter, Type S Modify, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1781","Inlets. Med Barrier, Type 1, J Bottom, =10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1782","Inlets. Med Barrier, Type 1, J Bottom, >10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1783","Inlets. Med Barrier, Type 1, J Bottom, <10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1785","Inlets. Med Barrier, Type 1, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1791","Inlets. Med Barrier, Type 2, =10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1792","Inlets. Med Barrier, Type 2, >10'",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1793","Inlets. Med Barrier, Type 2, J Bottom, <10'",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-1795","Inlets. Med Barrier, Type 2, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1799","Inlets. Med Barrier, Type 2, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1801","Inlets. Med Barrier, Type 1, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1802","Inlets. Med Barrier, Type 1, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1803","Inlets. Med Barrier, Type 1, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1804","Inlets. Med Barrier, Type 1, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1805","Inlets. Med Barrier, Type 1, Barrier",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1807","Inlets. Med Barrier, Type 1,  J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1809","Inlets. Med Barrier, Type 1, J Bottom, Modify",null,"EA",null,null,0,null,0,null,24.706645999999999,null,32.76]
[null,"0425-1811","Inlets. Med Barrier, Type 2, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1813","Inlets. Med Barrier, Type 2, J Bottom, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-1814","Inlets. Med Barrier, Type 2, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1815","Inlets. Med Barrier, Type 2, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1833","Inlets. Med Barrier, Type 2,  J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1841","Inlets. Med Barrier, Type 3, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1842","Inlets. Med Barrier, Type 3, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1843","Inlets. Med Barrier, Type 3, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1844","Inlets. Med Barrier, Type 3, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1845","Inlets. Med Barrier, Type 3, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1847","Inlets. Med Barrier, Type 3, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1848","Inlets. Med Barrier, Type 3, J Bottom, > 10, SPL",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1851","Inlets. Med Barrier, Type 4, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1852","Inlets. Med Barrier, Type 4, > 10",null,"EA",null,null,{"$f":"ROUND(F463*L463,0)","v":0},null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1853","Inlets. Med Barrier, Type 4, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1854","Inlets. Med Barrier, Type 4, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1855","Inlets. Med Barrier, Type 4, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1857","Inlets. Med Barrier, Type 4, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1859","Inlets. Med Barrier, Type 4, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1861","Inlets. Med Barrier, Type 5, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1862","Inlets. Med Barrier, Type 5, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1863","Inlets. Med Barrier, Type 5, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1864","Inlets. Med Barrier, Type 5, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1865","Inlets. Med Barrier, Type 5, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1869","Inlets. Med Barrier, Type 5, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1881","Inlets.  Barrier Wall, Rig, C & G, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1882","Inlets.  Barrier Wall, Rig, C & G, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1883","Inlets.  Barrier Wall, Rig, C & G, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1884","Inlets.  Barrier Wall, Rig, C & G, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1885","Inlets.  Barrier Wall, Rig, C & G, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1887","Inlets.  Barrier Wall, Rig, C & G, J Bottom, < 10, SPL",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1889","Inlets.  Barrier Wall, Rig, C & G, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1891","Inlets.  Barrier Wall, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1892","Inlets.  Barrier Wall, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1893","Inlets.  Barrier Wall, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1894","Inlets.  Barrier Wall, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1895","Inlets.  Barrier Wall, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1898","Inlets.  Barrier Wall, J Bottom, > 10, SPL",null,"EA",null,null,0,null,{"$f":"ROUND(F487*N487,0)","v":0},null,39.010100999999999,null,79.272727000000003]
[null,"0425-1899","Inlets.  Barrier Wall, Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1901","Inlets.  Special, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1902","Inlets.  Special, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1903","Inlets.  Special, J Bottom, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1904","Inlets.  Special, J Bottom, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1905","Inlets.  Special, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1909","Inlets.  Special. Modify",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1910","Inlets.  Closed Flume, N/A",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1921","Inlets.  Adjacent Barrier, <=10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1922","Inlets.  Adjacent Barrier, <10'",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-1923","Inlets.  Adjacent Barrier, J Bottom, <10'",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-1924","Inlets.  Adjacent Barrier, J Bottom, >10'",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-1925","Inlets.  Adjacent Barrier Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-41","Manholes, P-7, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-42","Manholes, P-7, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-2-43","Manholes, P-7, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-61","Manholes, P-8, < 10",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-62","Manholes, P-8, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,49.636364]
[null,"0425-2-63","Manholes, P-8, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-71","Manholes, J-7, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-2-72","Manholes, J-7, > 10",null,"EA",null,null,0,null,0,null,39.010100999999999,null,79.272727000000003]
[null,"0425-2-73","Manholes, J-7, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-91","Manholes, J-8, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-2-92","Manholes, J-8, > 10",null,"EA",null,null,0,null,0,null,25.746666000000001,null,52.32]
[null,"0425-2-93","Manholes, J-8, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-101","Manholes, Special, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-2-102","Manholes, Special, >10",null,"EA",null,null,0,null,0,null,25.746666000000001,null,32.76]
[null,"0425-2-103","Manholes, Special, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-2-110","Manholes, Repair ",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-3-41","Junction Box, Drainage, P-7, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-3-42","Junction Box, P-7, >10",null,"EA",null,null,0,null,0,null,25.746666000000001,null,32.76]
[null,"0425-3-43","Junction Box, Drainage, P-7, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-3-50","Junction Box, Repair",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-3-61","Junction Box, J-7, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-3-62","Junction Box, J-7, > 10",null,"EA",null,null,{"$f":"ROUND(F522*L522,0)","v":0},null,{"$f":"ROUND(F522*N522,0)","v":0},null,39.010100999999999,null,79.272727000000003]
[null,"0425-3-63","Junction Box, Drainage, J-7, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-3-81","Junction Box, Drainage, Special, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-3-82","Junction Box, Drainage, Special, > 10",null,"EA",null,null,0,null,0,null,25.746666000000001,null,32.76]
[null,"0425-3-83","Junction Box, Drainage, Special, Partial",null,"EA",null,null,0,null,0,null,24.706665999999998,null,32.76]
[null,"0425-3-91","Junction Box, Drainage, Utility, < 10",null,"EA",null,null,0,null,0,null,37.434344000000003,null,49.636364]
[null,"0425-3-92","Junction Box, Drainage, Utility, > 10",null,"EA",null,null,0,null,0,null,25.746666000000001,null,32.76]
[null,"0430-173-112","Pipe Culvert, Opt. Material, Round, 12\" GD",null,"LF",null,null,{"$f":"ROUND(F529*L529,0)","v":0},null,0,null,0.33333299999999999,null,1.17]
[null,"0430-173-115","Pipe Culvert, Opt. Material, Round, 15\" GD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-173-118","Pipe Culvert, Opt. Material, Round, 18\" GD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-173-124","Pipe Culvert, Opt. Material, Round, 24\" GD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-173-130","Pipe Culvert, Opt. Material, Round, 30\" GD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-173-136","Pipe Culvert, Opt. Material, Round, 36\" GD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-173-142","Pipe Culvert, Opt. Material, Round, 42\" GD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-173-148","Pipe Culvert, Opt. Material, Round, 48\" GD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-173-218","Pipe Culvert, Opt. Material, Other/Elliptical, 18\" GD",null,"LF",null,null,0,null,0,null,0.33333299999999999,null,1.17]
[null,"0430-174-112","Pipe Culvert, Opt. Material, Round, 12\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-115","Pipe Culvert, Opt. Material, Round, 15\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-118","Pipe Culvert, Opt. Material, Round, 18\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-124","Pipe Culvert, Opt. Material, Round, 24\" SD",null,"LF",null,null,{"$f":"ROUND(F541*L541,0)","v":0},null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-130","Pipe Culvert, Opt. Material, Round, 30\" SD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-174-136","Pipe Culvert, Opt. Material, Round, 36\" SD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-174-142","Pipe Culvert, Opt. Material, Round, 42\" SD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-174-148","Pipe Culvert, Opt. Material, Round, 48\" SD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-174-154","Pipe Culvert, Opt. Material, Round, 54\" SD",null,"LF",null,null,0,null,0,null,0.50303200000000003,null,2.6720139999999999]
[null,"0430-174-160","Pipe Culvert, Opt. Material, Round, 60\" SD",null,"LF",null,null,0,null,0,null,0.50303200000000003,null,2.6720139999999999]
[null,"0430-174-215","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 15\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-218","Pipe Culvert, Opt. Material, Other, Ellip/Arch 18\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-224","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 24\" SD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-174-230","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 30\" SD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-174-236","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 36\" SD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-174-242","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 42\" SD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-174-248","Pipe Culvert, Opt. Material, Other, Ellip/Arch, 48\" SD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-175-112","Pipe Culvert, Opt. Material, Round, 12\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-115","Pipe Culvert, Opt. Material, Round, 15\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-118","Pipe Culvert, Opt. Material, Round, 18\" SD/CD",null,"LF",null,null,0,null,{"$f":"ROUND(F557*N557,0)","v":0},null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-124","Pipe Culvert, Opt. Material, Round, 24\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-130","Pipe Culvert, Opt. Material, Round, 30\" SD/CD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-175-136","Pipe Culvert, Opt. Material, Round, 36\" SD/CD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-175-140","Pipe Culvert, Opt. Material, Round, 40\" SD/CD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-175-142","Pipe Culvert, Opt. Material, Round, 42\" SD/CD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-175-148","Pipe Culvert, Opt. Material, Round, 48\" SD/CD",null,"LF",null,null,0,null,0,null,0.45734799999999998,null,2.4179659999999998]
[null,"0430-175-154","Pipe Culvert, Opt. Material, Round, 54\" SD/CD",null,"LF",null,null,0,null,0,null,0.50303200000000003,null,2.6720139999999999]
[null,"0430-175-160","Pipe Culvert, Opt. Material, Round, 60\" SD/CD",null,"LF",null,null,0,null,0,null,0.56394500000000003,null,3.0107439999999999]
[null,"0430-175-166","Pipe Culvert, Opt. Material, Round, 66\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-172","Pipe Culvert, Opt. Material, Round, 72\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-178","Pipe Culvert, Opt. Material, Round, 78\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-184","Pipe Culvert, Opt. Material, Round, 84\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-196","Pipe Culvert, Opt. Material, Round, 96\" SD/CD",null,"LF",null,null,{"$f":"ROUND(F570*L570,0)","v":0},null,{"$f":"ROUND(F570*N570,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-199","Pipe Culvert, Opt. Material, Round, 99\" or Greater SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-215","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 15\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-218","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 18\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-224","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 24\" SD/CD",null,"LF",null,null,0,null,0,null,0.37088900000000002,null,1.8332999999999999]
[null,"0430-175-230","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 30\" SD/CD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-175-236","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 36\" SD/CD",null,"LF",null,null,0,null,0,null,0.39681499999999997,null,1.965929]
[null,"0430-175-242","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 42\" SD/CD",null,"LF",null,null,0,null,0,null,0.421815,null,2.2203729999999999]
[null,"0430-175-248","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 48\" SD/CD",null,"LF",null,null,0,null,0,null,0.45734799999999998,null,2.4179659999999998]
[null,"0430-175-254","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 54\" SD/CD",null,"LF",null,null,0,null,0,null,0.50303200000000003,null,2.6720139999999999]
[null,"0430-175-260","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 60\" SD/CD",null,"LF",null,null,{"$f":"ROUND(F580*L580,0)","v":0},null,0,null,0.56394500000000003,null,3.0107439999999999]
[null,"0430-175-266","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 66\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-272","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 72\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-175-299","Pipe Culvert, Opt. Material, Other-Ellip/Arch, 99\" SD/CD",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-025","U-Endwall, Std 261, 1:6 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-029","U-Endwall, Std 261, 1:6 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-033","U-Endwall, Std 261, 1:6 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-123","U-Endwall, Std 261, 1:4 Slope, 15\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-125","U-Endwall, Std 261, 1:4 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-129","U-Endwall, Std 261, 1:4 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-133","U-Endwall, Std 261, 1:4 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-223","U-Endwall, Std 261, 1:3 Slope, 15\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-225","U-Endwall, Std 261, 1:3 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-229","U-Endwall, Std 261, 1:3 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-233","U-Endwall, Std 261, 1:3 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-323","U-Endwall, Std 261, 1:2 Slope, 15\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-325","U-Endwall, Std 261, 1:2 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-610-329","U-Endwall, Std 261, 1:2 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-023","U-Endwall with Baffles, Std 261, 1:6 Slope, 15\" Pipe",null,"LF",null,null,{"$f":"ROUND(F598*L598,0)","v":0},null,{"$f":"ROUND(F598*N598,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-025","U-Endwall with Baffles, Std 261, 1:6 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-029","U-Endwall with Baffles, Std 261, 1:6 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-033","U-Endwall with Baffles, Std 261, 1:6 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-123","U-Endwall with Baffles, Std 261, 1:4 Slope, 15\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-125","U-Endwall with Baffles, Std 261, 1:4 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-129","U-Endwall with Baffles, Std 261, 1:4 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-133","U-Endwall with Baffles, Std 261, 1:6 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-223","U-Endwall with Baffles, Std 261, 1:3 Slope, 15\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-225","U-Endwall with Baffles, Std 261, 1:3 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-229","U-Endwall with Baffles, Std 261, 1:3 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-233","U-Endwall with Baffles, Std 261, 1:3 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-323","U-Endwall with Baffles/Grates, Std 261,1:2 Slope, 15\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-325","U-Endwall with Baffles/Grates, Std 261,1:2 Slope, 18\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-329","U-Endwall with Baffles/Grates, Std 261,1:2 Slope, 24\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-611-333","U-Endwall with Baffles/Grates, Std 261, 1:2 Slope, 30\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-025","U-Endwall with Grates, Std 261, 1:6 Slope, 18\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-029","U-Endwall with Grates, Std 261, 1:6 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-033","U-Endwall with Grates, Std 261, 1:6 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-125","U-Endwall with Baffles/Grates, Std 261,1:4 Slope, 18\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-129","U-Endwall with Baffles/Grates, Std 261,1:4 Slope, 24\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-133","U-Endwall with Baffles/Grates, Std 261,1:4 Slope, 30\" ",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-329","U-Endwall with Grates, Std 261, 1:2 Slope, 24\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-612-333","U-Endwall with Grates, Std 261, 1:2 Slope, 30\" Pipe",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-025","U-Endwall with Baffles/Grates, Std 261, 1:6 Slope, 18\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-029","U-Endwall with Baffles/Grates, Std 261, 1:6 Slope, 24\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-033","U-Endwall with Baffles/Grates, Std 261, 1:6 Slope, 30\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-123","U-Endwall with Baffles/Grates, Std 261, 1:4 Slope, 15\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-125","U-Endwall with Baffles/Grates, Std 261, 1:4 Slope, 18\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-133","U-Endwall with Baffles/Grates, Std 261, 1:4 Slope, 30\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-225","U-Endwall with Baffles/Grates, Std 261, 1:3 Slope, 18\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-233","U-Endwall with Baffles/Grates, Std 261, 1:3 Slope, 30\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-229","U-Endwall with Baffles/Grates, Std 261, 1:3 Slope, 24\"",null,"LF",null,null,{"$f":"ROUND(F630*L630,0)","v":0},null,{"$f":"ROUND(F630*N630,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-325","U-Endwall with Baffles/Grates, Std 261, 1:2 Slope, 18\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-613-333","U-Endwall with Baffles/Grates, Std 261, 1:2 Slope, 30\"",null,"LF",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-12","Manatee Gate for 12\" Pipe",null,"EA",null,null,{"$f":"ROUND(F633*L633,0)","v":0},null,{"$f":"ROUND(F633*N633,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-18","Manatee Gate for 18\" Pipe",null,"EA",null,null,{"$f":"ROUND(F634*L634,0)","v":0},null,{"$f":"ROUND(F634*N634,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-24","Manatee Gate for 24\" Pipe",null,"EA",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-30","Manatee Gate for 30\" Pipe",null,"EA",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-36","Manatee Gate for 36\" Pipe",null,"EA",null,null,{"$f":"ROUND(F637*L637,0)","v":0},null,{"$f":"ROUND(F637*N637,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-42","Manatee Gate for 42\" Pipe",null,"EA",null,null,{"$f":"ROUND(F638*L638,0)","v":0},null,{"$f":"ROUND(F638*N638,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-48","Manatee Gate for 48\" Pipe",null,"EA",null,null,{"$f":"ROUND(F639*L639,0)","v":0},null,{"$f":"ROUND(F639*N639,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-885-60","Manatee Gate for 60\" Pipe",null,"EA",null,null,{"$f":"ROUND(F640*L640,0)","v":0},null,{"$f":"ROUND(F640*N640,0)","v":0},null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-886-24","Manatee Grate for 24\" Pipe, Unhinged",null,"EA",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-886-36","Manatee Grate for 36\", Unhinged",null,"EA",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0430-886-60","Manatee Grate for 60\" or Greater Pipe, Unhinged",null,"EA",null,null,0,null,0,null,0.48144500000000001,null,3.9349099999999999]
[null,"0444-74-1","Deep Well Injection Box, Structure With No Outflow",null,"EA",null,null,0,null,0,null,25.746666000000001,null,32.76]
[null,"0444-74-2","Deep Well Injection Box, Structure With Outflow",null,"EA",null,null,{"$f":"ROUND(F645*L645,0)","v":0},null,{"$f":"ROUND(F645*N645,0)","v":0},null,25.746666000000001,null,32.76]
[null,"0450-1-4","Prestressed Beams, V",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-1-5","Prestressed Beams, VI",null,"LF",null,null,0,null,0,null,9.7254999999999994E-2,null,0.53315900000000005]
[null,"0450-1-7","Prestressed Beams, Special",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-1-72","Prestressed Beams, Bulb T - 72",null,"LF",null,null,0,null,0,null,8.6032999999999998E-2,null,0.47164099999999998]
[null,"0450-1-78","Prestressed Beams, Bulb T - 78",null,"LF",null,null,0,null,0,null,8.2848000000000005E-2,null,0.454175]
[null,"0450-1-203","Prestressed Beams, Type IV, Modified",null,"LF",null,null,0,null,0,null,0.122462,null,0.28659000000000001]
[null,"0450-1-250","Prestressed Beams, Inverted T 20",null,"LF",null,null,0,null,0,null,9.9819000000000005E-2,null,0.17618700000000001]
[null,"0450-1-251","Prestressed Beams, Inverted T Mod Form FIB. 26.5\"",null,"LF",null,null,0,null,0,null,9.9819000000000005E-2,null,0.17618700000000001]
[null,"0450-2-36","Prestressed Beams, FL I Beam 36\"",null,"LF",null,null,0,null,0,null,0.14202400000000001,null,0.254357]
[null,"0450-2-45","Prestressed Beams, FL I Beam 45\"",null,"LF",null,null,0,null,0,null,0.106518,null,0.19076799999999999]
[null,"0450-2-54","Prestressed Beams, FL I Beam 54\"",null,"LF",null,null,0,null,0,null,0.122462,null,0.286659]
[null,"0450-2-63","Prestressed Beams, FL I Beam 63\"",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-2-72","Prestressed Beams, FL I Beam 72\"",null,"LF",null,null,0,null,0,null,9.7254999999999994E-2,null,0.53315900000000005]
[null,"0450-2-78","Prestressed Beams, FL I Beam 78\"",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-2-84","Prestressed Beams, FL I Beam 84\"",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-2-96","Prestressed Beams, FL I Beam 96\"",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-2-178","Prest. Beams, FL I Beam 78\" Modified With Post Tens.",null,"LF",null,null,0,null,0,null,0.13475200000000001,null,0.72809699999999999]
[null,"0450-3-11","Prestressed Slab Units, 48\" X 12\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-15","Prestressed Slab Units, 48\" X 15\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-21","Prestressed Slab Units, 60\" X 12\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-22","Prestressed Slab Units, 60\" X 16\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-25","Prestressed Slab Units, 60\" X 15\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-33","Prestressed Slab Units, 96\" X 10\"",null,"LF",null,null,{"$f":"ROUND(F668*L668,0)","v":0},null,{"$f":"ROUND(F668*N668,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0450-3-41","Prestressed Slab Units, 72\" X 12\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-62","Prestressed Slab Units, 54\" X 16\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-72","Prestressed Slab Units, 57\" X 16\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-91","Prestressed Slab Units, Variable Width 30\"- 47\" Thick 12\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-3-95","Prestressed Slab Units, Variable Width 30\"- 47\" Thick 15\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-4-1","Prestressed Beams FL U-Beam, 48",null,"LF",null,null,0,null,0,null,0.104528,null,0.56066300000000002]
[null,"0450-4-2","Prestressed Beams FL U-Beam, 54",null,"LF",null,null,0,null,0,null,0.104528,null,0.56066300000000002]
[null,"0450-4-3","Prestressed Beams FL U-Beam, 63",null,"LF",null,null,0,null,{"$f":"ROUND(F676*N676,0)","v":0},null,7.6504000000000003E-2,null,0.41284500000000002]
[null,"0450-4-4","Prestressed Beams FL U-Beam, 72",null,"LF",null,null,{"$f":"ROUND(F677*L677,0)","v":0},null,{"$f":"ROUND(F677*N677,0)","v":0},null,7.6504000000000003E-2,null,0.41284500000000002]
[null,"0450-4-15","Prestressed Beams FL U-Beam,",null,"LF",null,null,0,null,0,null,7.6504000000000003E-2,null,0.41284500000000002]
[null,"0450-7-6","Curved Precast Spliced U-Girder, U90-4",null,"LF",null,null,{"$f":"ROUND(F679*L679,0)","v":0},null,{"$f":"ROUND(F679*N679,0)","v":0},null,7.6504000000000003E-2,null,0.41284500000000002]
[null,"0450-8-11","Prestressed Beam FL Slab Beam, Depth 12\", Width 48-51\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-8-12","Prestressed Beams FL Slab Beam, Depth 12\", Width 52-54\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-8-13","Prestressed Beams FL Slab Beam, Depth 12\", Width 55-57\"",null,"LF",null,null,{"$f":"ROUND(F682*L682,0)","v":0},null,{"$f":"ROUND(F682*N682,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0450-8-14","Prestressed Beam FL Slab Beam, Depth 12\", Width 58-60\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-8-21","Prestressed Beams FL Slab Beam, Depth 15\", Width 48-51\"",null,"LF",null,null,{"$f":"ROUND(F684*L684,0)","v":0},null,{"$f":"ROUND(F684*N684,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0450-8-23","Prestressed Beams FL Slab Beam, Depth 15\", Width 55-57\"",null,"LF",null,null,{"$f":"ROUND(F685*L685,0)","v":0},null,{"$f":"ROUND(F685*N685,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0450-8-24","Prestressed Beams FL Slab Beam, Depth 15\", Width 58-60\"",null,"LF",null,null,{"$f":"ROUND(F686*L686,0)","v":0},null,{"$f":"ROUND(F686*N686,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0450-8-31","Prestressed Beams FL Slab Beam, Depth 18\", Width 48-51\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-8-32","Prestressed Beams FL Slab Beam, Depth 18\", Width 52-54\"",null,"LF",null,null,0,null,0,null,0.159776,null,0.28614899999999999]
[null,"0450-8-33","Prestressed Beams FL Slab Beam, Depth 18\", Width 55-57\"",null,"LF",null,null,{"$f":"ROUND(F689*L689,0)","v":0},null,{"$f":"ROUND(F689*N689,0)","v":0},null,0.159776,null,0.28614899999999999]
[null,"0455-14-2","Concrete Sheet Piling, 8 X 30",null,"LF",null,null,0,null,0,null,0.31563999999999998,null,0.57874000000000003]
[null,"0455-14-3","Concrete Sheet Piling, 10 X 30",null,"LF",null,null,0,null,0,null,0.31563999999999998,null,0.57874000000000003]
[null,"0455-14-4","Concrete Sheet Piling, 12 X 30",null,"LF",null,null,0,null,0,null,0.27994000000000002,null,0.64024999999999999]
[null,"0455-14-5","Concrete Sheet Piling, Special",null,"LF",null,null,0,null,0,null,0.31563999999999998,null,0.57874000000000003]
[null,"0455-14-23","Concrete Sheet Piling, CFRP/GFRP 10\" X 30\" w/FRP Strand & Reinforcing",null,"LF",null,null,0,null,0,null,0.27994000000000002,null,0.64024999999999999]
[null,"0455-14-24","Concrete Sheet Piling, 12 X 30 with FRP Strand and Reinforcing",null,"LF",null,null,{"$f":"ROUND(F695*L695,0)","v":0},null,{"$f":"ROUND(F695*N695,0)","v":0},null,0.27994000000000002,null,0.64024999999999999]
[null,"0455-34-1","Prestressed Concrete Pilng, 12\" Square",null,"LF",null,null,0,null,0,null,9.3269000000000005E-2,null,0.21138000000000001]
[null,"0455-34-2","Prestressed Concrete Pilng, 14\" Square",null,"LF",null,null,0,null,0,null,9.3269000000000005E-2,null,0.21138000000000001]
[null,"0455-34-3","Prestressed Concrete Pilng, 18\" Square",null,"LF",null,null,0,null,0,null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-4","Prestressed Concrete Pilng, 20\" Square",null,"LF",null,null,0,null,0,null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-5","Prestressed Concrete Pilng, 24\" Square",null,"LF",null,null,0,null,0,null,0.16248799999999999,null,0.57325700000000002]
[null,"0455-34-6","Prestressed Concrete Pilng, 30\" Square",null,"LF",null,null,0,null,0,null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-34-7","Prestressed Concrete Pilng, 36\" Square",null,"LF",null,null,{"$f":"ROUND(F702*L702,0)","v":0},null,0,null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-34-8","Concrete Piling Prestressed, Special",null,"LF",null,null,0,null,0,null,0.223528,null,0.84603300000000004]
[null,"0455-34-23","Prestressed Concrete Pilng, 18\" SQ with FRP Strand and Reinf",null,"LF",null,null,{"$f":"ROUND(F704*L704,0)","v":0},null,{"$f":"ROUND(F704*N704,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-25","Prestressed Concrete Piling 24\" SQ W/FRP or Stainless Steel, Strand & Reinf",null,"LF",null,null,{"$f":"ROUND(F705*L705,0)","v":0},null,{"$f":"ROUND(F705*N705,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-103","Prestressed Concrete Piling, Includes 100% Dynamic Testing, Internal Gauges, 18\" SQ",null,"LF",null,null,{"$f":"ROUND(F706*L706,0)","v":0},null,{"$f":"ROUND(F706*N706,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-105","Prestressed Concrete Piling, Includes 100% Dynamic Testing, Internal Gauges, 24\" SQ",null,"LF",null,null,{"$f":"ROUND(F707*L707,0)","v":0},null,{"$f":"ROUND(F707*N707,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-106","Prestressed Concrete Piling, Includes 100% Dynamic Testing, Internal Gauges, 30\" SQ",null,"LF",null,null,{"$f":"ROUND(F708*L708,0)","v":0},null,{"$f":"ROUND(F708*N708,0)","v":0},null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-34-107","Prestressed Concrete Piling, Includes 100% Dynamic Testing, Internal Gauges, 36\" SQ",null,"LF",null,null,{"$f":"ROUND(F709*L709,0)","v":0},null,{"$f":"ROUND(F709*N709,0)","v":0},null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-34-120","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 18\" Diam",null,"LF",null,null,0,null,0,null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-121","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 20\" Diam",null,"LF",null,null,{"$f":"ROUND(F711*L711,0)","v":0},null,{"$f":"ROUND(F711*N711,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-125","Prestressed Concrete Piling, Includes 100% Dynamic Testing, Internal Gauges, 24\" SQ W/FRP or Stainless Steel Strand Reinforcing",null,"LF",null,null,0,null,0,null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-203","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 18\" SQ",null,"LF",null,null,{"$f":"ROUND(F713*L713,0)","v":0},null,{"$f":"ROUND(F713*N713,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-205","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 24\" SQ",null,"LF",null,null,{"$f":"ROUND(F714*L714,0)","v":0},null,{"$f":"ROUND(F714*N714,0)","v":0},null,0.16442200000000001,null,0.56067699999999998]
[null,"0455-34-206","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 30\" SQ",null,"LF",null,null,{"$f":"ROUND(F715*L715,0)","v":0},null,{"$f":"ROUND(F715*N715,0)","v":0},null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-34-207","Prestressed Concrete Piling, Includes 100% Dynamic Testing, External Gauges, 36\" SQ",null,"LF",null,null,{"$f":"ROUND(F716*L716,0)","v":0},null,{"$f":"ROUND(F716*N716,0)","v":0},null,0.20117499999999999,null,0.88319199999999998]
[null,"0455-35-1","Steel Piling, HP 8 X 36",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-3","Steel Piling, HP 10 X 42",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-4","Steel Piling, HP 12 X 53",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-5","Steel Piling, HP 14 X 73",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-6","Steel Piling, HP 14 X 89",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-7","Steel Piling, HP 14 X 102",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-8","Steel Piling, HP 14 X 117",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-9","Steel Piling, Special",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-10","Steel Piling, HP 16 X 101",null,"LF",null,null,{"$f":"ROUND(F725*L725,0)","v":0},null,{"$f":"ROUND(F725*N725,0)","v":0},null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-11","Steel Piling, HP 12 X 74",null,"LF",null,null,{"$f":"ROUND(F726*L726,0)","v":0},null,{"$f":"ROUND(F726*N726,0)","v":0},null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-12","Steel Piling, HP 16 X 88",null,"LF",null,null,{"$f":"ROUND(F727*L727,0)","v":0},null,{"$f":"ROUND(F727*N727,0)","v":0},null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-13","Steel Piling, HP 16 X 121",null,"LF",null,null,{"$f":"ROUND(F728*L728,0)","v":0},null,{"$f":"ROUND(F728*N728,0)","v":0},null,9.2850000000000002E-2,null,0.211725]
[null,"0455-35-20","Steel Piling, 18\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.14369699999999999,null,0.391735]
[null,"0455-35-21","Steel Piling, 20\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.14369699999999999,null,0.391735]
[null,"0455-35-22","Steel Piling, 24\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.14369699999999999,null,0.391735]
[null,"0455-35-23","Steel Piling, 30\" Dia. Pipe",null,"LF",null,null,{"$f":"ROUND(F732*L732,0)","v":0},null,{"$f":"ROUND(F732*N732,0)","v":0},null,0.14369699999999999,null,0.391735]
[null,"0455-43-25","Test Piles-Prestressed Concrete 24\" SQ W/FRP or Stainless Steel Strand & Reinf",null,"LF",null,null,0,null,0,null,0.14369699999999999,null,0.391735]
[null,"0455-88-1","Drilled Shaft, 24\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-88-2","Drilled Shaft, 30\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-88-3","Drilled Shaft, 36\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-88-4","Drilled Shaft, 42\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-88-5","Drilled Shaft, 48\" Dia. ",null,"LF",null,null,0,null,0,null,1.207133,null,4.6994559999999996]
[null,"0455-88-6","Drilled Shaft, 60\" Dia. ",null,"LF",null,null,0,null,0,null,1.5784499999999999,null,6.1084750000000003]
[null,"0455-88-7","Drilled Shaft, 72\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-88-8","Drilled Shaft, 54\" Dia. ",null,"LF",null,null,0,null,0,null,1.207133,null,4.9032559999999998]
[null,"0455-88-9","Drilled Shaft, 66\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-88-15","Drilled Shaft, 84\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-88-19","Drilled Shaft, 90\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-88-20","Drilled Shaft, 108\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-88-21","Drilled Shaft, 96\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.5737500000000004]
[null,"0455-107-1","Drilled Shaft Casing, 24\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-2","Drilled Shaft Casing, 30\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-3","Drilled Shaft Casing, 36\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-4","Drilled Shaft Casing, 42\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-5","Drilled Shaft Casing, 48\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-6","Drilled Shaft Casing, 60\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-7","Drilled Shaft Casing, 72\" Dia. ",null,"LF",null,null,0,null,0,null,0.83567800000000003,null,3.2900170000000002]
[null,"0455-107-8","Drilled Shaft Casing, 54\" Dia. ",null,"LF",null,null,0,null,0,null,1.207133,null,4.9032559999999998]
[null,"0455-107-9","Drilled Shaft Casing, 66\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.59375]
[null,"0455-107-18","Drilled Shaft Casing, 84\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.59375]
[null,"0455-107-19","Drilled Shaft Casing, 90\" Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.59375]
[null,"0455-107-20","Drilled Shaft Casing, 108 Dia. ",null,"LF",null,null,0,null,0,null,1.857,null,6.59375]
[null,"0455-107-21","Drilled Shaft Casing, 96\" Dia. ",null,"LF",null,null,0,null,0,null,1.207133,null,4.9032559999999998]
[null,"0455-143-1","Test Piles - Precast Concrete, 12\" Square",null,"LF",null,null,0,null,0,null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-2","Test Piles - Precast Concrete, 14\" Square",null,"LF",null,null,0,null,0,null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-3","Test Piles - Precast Concrete, 18\" Square",null,"LF",null,null,0,null,0,null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-4","Test Piles - Precast Concrete, 20\" Square",null,"LF",null,null,0,null,0,null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-5","Test Piles - Precast Concrete, 24\" Square",null,"LF",null,null,0,null,0,null,0.65768800000000005,null,2.3212600000000001]
[null,"0455-143-6","Test Piles - Precast Concrete, 30\" Square",null,"LF",null,null,0,null,0,null,0.77375000000000005,null,3.3952599999999999]
[null,"0455-143-7","Test Piles - Precast Concrete, 36\" Square",null,"LF",null,null,0,null,0,null,0.77375000000000005,null,3.3952599999999999]
[null,"0455-143-23","Test Piles - Precast Concrete, 18\" Square with FRP Strands and Reinforcing",null,"LF",null,null,{"$f":"ROUND(F767*L767,0)","v":0},null,{"$f":"ROUND(F767*N767,0)","v":0},null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-25","Test Piles - Prestressed Concrete, 24\" SQ W/ FRP or Stainless Steel Strand & Reinforcing",null,"LF",null,null,{"$f":"ROUND(F768*L768,0)","v":0},null,{"$f":"ROUND(F768*N768,0)","v":0},null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-103","Test Piles - Prestressed Concrete, 100% Dynamic Testing with Internal Gauges, 18\" Square",null,"LF",null,null,{"$f":"ROUND(F769*L769,0)","v":0},null,{"$f":"ROUND(F769*N769,0)","v":0},null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-105","Test Piles - Prestressed Concrete, 100% Dynamic Testing with Internal Gauges, 24\" Square",null,"LF",null,null,{"$f":"ROUND(F770*L770,0)","v":0},null,{"$f":"ROUND(F770*N770,0)","v":0},null,0.65768800000000005,null,2.3212600000000001]
[null,"0455-143-203","Test Piles - Prestressed Concrete, 100% Dynamic Testing with External Gauges, 18\" Square",null,"LF",null,null,{"$f":"ROUND(F771*L771,0)","v":0},null,{"$f":"ROUND(F771*N771,0)","v":0},null,0.87691699999999995,null,2.5540829999999999]
[null,"0455-143-105","Test Piles - Prestressed Concrete, 100% Dynamic Testing with External Gauges, 24\" Square",null,"LF",null,null,0,null,0,null,0.65768800000000005,null,2.3212600000000001]
[null,"0455-144-1","Test Piles - Steel, HP 8 X 36",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-2","Test Piles - Steel, HP 10 X 36",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-3","Test Piles - Steel, HP 10 X 42",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-4","Test Piles - Steel, HP 12 X 53",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-5","Test Piles - Steel, HP 14 X 73",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-6","Test Piles - Steel, HP 14X 89",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-8","Test Piles - Steel, HP 14 X 117",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-9","Test Piles - Steel, Special",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-20","Test Piles - Steel, 18\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-21","Test Piles - Steel, 20\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-22","Test Piles - Steel, 24\" Dia. Pipe",null,"LF",null,null,0,null,{"$f":"ROUND(F783*N783,0)","v":0},null,0.52229199999999998,null,1.3668439999999999]
[null,"0455-144-23","Test Piles - Steel, 30\" Dia. Pipe",null,"LF",null,null,0,null,0,null,0.52229199999999998,null,1.3668439999999999]
[null,"0460-1-1","Structural Steel - Rehab, Carbon",null,"LB",null,null,0,null,0,null,5.0369999999999998E-3,null,7.5300000000000002E-3]
[null,"0460-1-2","Structural Steel - (Low Alloy)",null,"LB",null,null,0,null,0,null,5.8699999999999996E-4,null,3.3370000000000001E-3]
[null,"0460-1-3","Structural Steel - Rehab, Shoe Assemblies",null,"LB",null,null,0,null,0,null,5.0369999999999998E-3,null,7.5300000000000002E-3]
[null,"0460-1-5","Structural Steel - Rehab, Bascule Leaves",null,"LB",null,null,0,null,0,null,1.1254999999999999E-2,null,4.2509999999999999E-2]
[null,"0460-1-11","Structural Steel - Rehab, Screws, Bolts & Washers, ass.",null,"LB",null,null,0,null,0,null,1.2859000000000001E-2,null,2.2985999999999999E-2]
[null,"0460-1-13","Structural Steel - Rehab - Bolt, Nut, Wash. & Plate",null,"LB",null,null,0,null,0,null,1.2859000000000001E-2,null,2.2985999999999999E-2]
[null,"0460-1-15","Structural Steel - Rehab, Misc.",null,"LB",null,null,0,null,0,null,4.4739999999999997E-3,null,1.2637000000000001E-2]
[null,"0460-2-1","Structural Steel - Carbon*",null,"LS/Lbs",null,null,0,null,0,null,9.7799999999999992E-4,null,3.5630000000000002E-3]
[null,"0460-2-2","Structural Steel - Low Alloy*",null,"LS/Lbs",null,null,0,null,0,null,5.8699999999999996E-4,null,3.3370000000000001E-3]
[null,"0460-2-3","Structural Steel - Rehab, Shoe Assemblies*",null,"LS/Lbs",null,null,0,null,0,null,5.0369999999999998E-3,null,7.5300000000000002E-3]
[null,"0460-2-5","Structural Steel - Bascule Leaves*",null,"LS/Lbs",null,null,{"$f":"ROUND(F795*L795,0)","v":0},null,0,null,1.286E-3,null,4.8580000000000003E-3]
[null,"0460-2-6","Structural Steel - Bascule Piers*",null,"LS/Lbs",null,null,0,null,0,null,7.718E-3,null,1.8744E-2]
[null,"0460-2-15","Structural Steel - Miscellaneous*",null,"LS/Lbs",null,null,0,null,0,null,2.6072999999999999E-2,null,3.1633000000000001E-2]
[null,"0460-2-20","Structural Steel - New/Widening, Weathering*",null,"LS/Lbs",null,null,0,null,0,null,2.6072999999999999E-2,null,3.1633000000000001E-2]
[null,"0460-6-1","Ladders & Platforms, New",null,"LB",null,null,0,null,0,null,4.5019999999999998E-2,null,4.9160000000000002E-2]
[null,"0460-6-2","Ladders & Platforms, Rehab",null,"LB",null,null,0,null,0,null,4.5019999999999998E-2,null,4.9160000000000002E-2]
[null,"0460-15","Stainless Steel Vermin Guard-for Maint. or Rehab",null,"LB",null,null,0,null,0,null,4.4739999999999997E-3,null,1.2637000000000001E-2]
[null,"0460-94","Structural Steel Repair- Welds",null,"LF",null,null,0,null,0,null,2.6072999999999999E-2,null,3.1633000000000001E-2]
[null,"0460-95","Structural Steel Repair",null,"LB",null,null,0,null,0,null,2.6072999999999999E-2,null,3.1633000000000001E-2]
[null,"0520-1-7","Concrete Curb & Gutter, Type E",null,"LF",null,null,0,null,0,null,5.8390999999999998E-2,null,3.8082999999999999E-2]
[null,"0520-1-8","Concrete Curb & Gutter, Special",null,"LF",null,null,0,null,0,null,0.22159499999999999,null,5.5384000000000003E-2]
[null,"0520-1-10","Concrete Curb & Gutter, Type F",null,"LF",null,null,0,null,0,null,6.1610999999999999E-2,null,4.0183000000000003E-2]
[null,"0520-2-1","Concrete Curb, Type A",null,"LF",null,null,0,null,0,null,6.1628000000000002E-2,null,4.0194000000000001E-2]
[null,"0520-2-2","Concrete Curb, Type B",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0520-2-4","Concrete Curb, Type D",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0520-2-8","Concrete Curb, Type RA",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0520-2-9","Concrete Curb, Special",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0520-3","Valley Gutter Concrete",null,"LF",null,null,0,null,0,null,0.21895000000000001,null,4.7600000000000003E-2]
[null,"0520-5-11","Traffic Sep. Conc.Type I, 4 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,3.1732999999999997E-2]
[null,"0520-5-12","Traffic Sep. Conc.Type I, 6 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,4.7600000000000003E-2]
[null,"0520-5-16","Traffic Sep. Conc.Type I, 8.5 Wide ",null,"LF",null,null,0,null,0,null,0.27293299999999998,null,0]
[null,"0520-5-21","Traffic Sep. Conc.Type II, 4 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,3.1732999999999997E-2]
[null,"0520-5-22","Traffic Sep. Conc.Type II, 6 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,4.7600000000000003E-2]
[null,"0520-5-26","Traffic Sep. Conc.Type II, 8.5 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,4.7600000000000003E-2]
[null,"0520-5-41","Traffic Sep. Conc.Type IV, 4 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,3.1732999999999997E-2]
[null,"0520-5-42","Traffic Sep. Conc.Type IV, 6 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,4.7600000000000003E-2]
[null,"0520-5-46","Traffic Sep. Conc.Type IV, 8.5 Wide ",null,"LF",null,null,0,null,0,null,0.27293299999999998,null,0]
[null,"0520-5-51","Traffic Sep. Conc.Type V, 4 Wide ",null,"LF",null,null,0,null,0,null,0.136467,null,3.1732999999999997E-2]
[null,"0520-5-52","Traffic Sep. Conc.Type V, 6 Wide",null,"LF",null,null,0,null,0,null,0.136467,null,4.7600000000000003E-2]
[null,"0520-6","Shoulder Gutter Concrete",null,"LF",null,null,0,null,0,null,0.12379999999999999,null,7.9333000000000001E-2]
[null,"0520-7-1","Granite Curb, Furnish & Install",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0520-7-2","Granite Curb, Reset",null,"LF",null,null,0,null,0,null,0.29993199999999998,null,0]
[null,"0521-1","Median Concrete Barrier Wall",null,"LF",null,null,0,null,0,null,9.2850000000000002E-2,null,8.3299999999999999E-2]
[null,"0521-1-1","Barrier Wall Concrete, Precast",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-1-11","Median Concrete Barrier, 38\" Height",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-1-12","Median Concrete Barrier, Short Grade-Separated",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-1-13","Median Concrete Barrier, Tall Grade-Separated",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-1-14","Median Concrete Barrier, variable section width for sign or pier shielding",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-5-1","Concrete Traffic Rail, Brg., 32 F-Shape",null,"LF",null,null,0,null,0,null,0.34375299999999998,null,0.156332]
[null,"0521-5-2","Concrete Traffic Rail, Brg., 42 F-Shape",null,"LF",null,null,0,null,0,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-3","Concrete Traffic Rail, Brg., 32 F-Med. Dbl.",null,"LF",null,null,0,null,0,null,0.31065700000000002,null,0.23063900000000001]
[null,"0521-5-4","Concrete Traffic Rail, Brg., 32 Vert. Face",null,"LF",null,null,0,null,0,null,0.34375299999999998,null,0.156332]
[null,"0521-5-5","Concrete Traffic Rail, Brg., 42 Vert. Face",null,"LF",null,null,0,null,0,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-6","Concrete Traffic Rail, Brg., Corral with Curb",null,"LF",null,null,0,null,0,null,1.2696670000000001,null,0]
[null,"0521-5-7","Concrete Traffic Rail, Brg., Corral without Curb",null,"LF",null,null,0,null,0,null,1.2696670000000001,null,0]
[null,"0521-5-8","Concrete Traffic Rail, Brg., Retro-Vert. Face",null,"LF",null,null,0,null,0,null,0.44625399999999998,null,0.28482800000000003]
[null,"0521-5-9","Concrete Traffic Rail, Brg., Special",null,"LF",null,null,0,null,0,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-10","Concrete rg., Brg., Repair Existing",null,"LF",null,null,0,null,0,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-12","Concrete Traffic Rail, Brg, 36 Median Single-Slope, Double Face",null,"EA",null,null,null,null,null,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-13","Concrete Traffic Rail, Brg, 36 Single-Slope",null,"LF",null,null,{"$f":"ROUND(F844*L844,0)","v":0},null,{"$f":"ROUND(F844*N844,0)","v":0},null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-14","Concrete Traffic Railing, Brg, 42\" Single-Slope",null,"LF",null,null,0,null,0,null,0.68262100000000003,null,0.24072499999999999]
[null,"0521-5-20","Concrete rg., Brg., F Shaped W/Snd, 8",null,"LF",null,null,0,null,0,null,0.34375299999999998,null,0.156332]
[null,"0521-5-22","Concrete Traffic Railing, Brg, 8'0\" Noise Wall",null,"LF",null,null,0,null,0,null,0.34375299999999998,null,0.156332]
[null,"0521-6-11","Concrete Parapet, Pedestrian/Bicycle, 27\" Height",null,"LF",null,null,0,null,0,null,0.85680000000000001,null,0]
[null,"0521-6-12","Concrete Parapet, Pedestrian/Bicycle, 42\" Height",null,"LF",null,null,0,null,0,null,0.85680000000000001,null,0]
[null,"0521-6-15","Concrete Parapet, Ped/Bicycle, 26\" Height w Stone Cap",null,"LF",null,null,0,null,0,null,0.85680000000000001]
[null,"0521-6-31","Concrete Parapet, Retaining Wall Mtd. W/SW 72\" Height",null,"LF",null,null,0,null,0,null,1.7136,null,0]
[null,"0521-7-1","Concrete Taffic Rail Barrier, Ret. Wall Sys/Snd",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.48099999999999998]
[null,"0521-8-1","Concrete Taffic Rail Barrier, Ret. Wall 32\" F Shp",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-2","Concrete Taffic Rail Barrier, Ret. Wall 42\" F Shp",null,"LF",null,null,0,null,0,null,0.92849999999999999,null,0.36075000000000002]
[null,"0521-8-3","Concrete Taffic Rail Barrier, Ret. Wall 32\" V Shp",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-4","Concrete Taffic Rail Bar., Ret. Wall, Mtd. SS, 42\" Vert. F ",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-5","Concrete Taffic Rail Bar.,W Junct. Slab, Corral W Curb ",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-6","Concrete Taffic Rail Bar.,W Junct. Slab, Corral without Curb ",null,"LF",null,null,{"$f":"ROUND(F858*L858,0)","v":0},null,{"$f":"ROUND(F858*N858,0)","v":0},null,1.238,null,0.48099999999999998]
[null,"0521-8-7","Concrete Traffic Railing Barrier, W Junction Slab, 36\", Single Slope",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-8","Concrete Barrier, W Junction Slab, 42\" Single Slope",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-8-11","Concrete Traffic Railing, W Junction Slab, 8'0\" Noise Wall",null,"LF",null,null,0,null,0,null,1.238,null,0.48099999999999998]
[null,"0521-9-1","Opaque Visual Barrier, Index 521-010 Concrete",null,"LF",null,null,0,null,0,null,6.1899999999999997E-2,null,8.4532999999999997E-2]
[null,"0521-72-2","Shoulder Concrete Barrier Wall, Box Culvert",null,"LF",null,null,0,null,0,null,1.071,null,0]
[null,"0521-72-3","Shoulder Concrete Barrier Wall, Rigid-Shoulder",null,"LF",null,null,0,null,{"$f":"ROUND(F864*N864,0)","v":0},null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-4","Shoulder Concrete Barrier Wall, Rigid-Retain",null,"LF",null,null,0,null,0,null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-5","Shoulder Concrete Barrier Wall, Rigid-C & G",null,"LF",null,null,0,null,0,null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-7","Shoulder Concrete Barrier Wall, Rigid-Shoulder",null,"LF",null,null,0,null,0,null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-10","Shoulder Concrete Barrier Wall, Rigid-Shldr 42\",Index411",null,"LF",null,null,0,null,0,null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-11","Shoulder Concrete Barrier Wall, Rigid-Shldr 54\",Index411",null,"LF",null,null,0,null,0,null,0.33684999999999998,null,0.10813300000000001]
[null,"0521-72-20","Shoulder Concrete Barrier Wall, F Shape, 8' Snd Wall",null,"LF",null,null,{"$f":"ROUND(F870*L870,0)","v":0},null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-21","Shoulder Concrete Barrier Wall, F Shape, 10' Snd Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-22","Shoulder Concrete Barrier Wall, F Shape, 12' Snd Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-23","Shoulder Concrete Barrier Wall, F Shape, 14' Snd Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-24","Shoulder Concrete Barrier Wall, 8' Noise Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-27","Shoulder Concrete Barrier Wall, 14' Noise Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-40","Shoulder Concrete Barrier Wall, 38\" or 44\" Height",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-41","Shoulder Concrete Barrier, Retaining Section",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-42","Shoulder Concrete Barrier, 38\" Trench Footing Section",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-43","Shoulder Concrete Barrier, Curb and Gutter Barrier",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-44","Shoulder Concrete Barrier, 44\" Pier Protection Barrier/Crash, Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-56","Shoulder Concrete Barrier, 56\" Pier Protection Barrier/Crash, Wall",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-60","Shoulder Concrete Barrier, 38\" Wall Shielding Barrier",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-72-61","Shoulder Concrete Barrier, Vairable Width for Wall or Sign Shielding",null,"LF",null,null,0,null,0,null,1.4279999999999999,null,0.64133300000000004]
[null,"0521-73","Concrete Barrier Wall Removal",null,"LF",null,null,0,null,0,null,0.24759999999999999,null,1.448267]
[null,"0522-1","Sidewalk Concrete, 4\" Thick",null,"SY",null,null,0,null,0,null,0.32533299999999998,null,0]
[null,"0522-2","Sidewalk Concrete, 6\" Thick",null,"SY",null,null,0,null,0,null,0.32533299999999998,null,0]
[null,"0522-3","Bus Bay/Boarding Pad - Concrete",null,"SY",null,null,0,null,0,null,0.32533299999999998,null,0]
[null,"0522-4","Bus Shelter Pad - Concrete",null,"SY",null,null,0,null,0,null,0.32533299999999998,null,0]
[null,"0524-1-1","Concrete Ditch Pavement, NR, 3",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-2","Concrete Ditch Pavement, NR, 4",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-3","Concrete Ditch Pavement, NR, 5",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-4","Concrete Ditch Pavement, NR, 6",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-19","Concrete Ditch Pavement, 3, Reinforced",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-29","Concrete Ditch Pavement, 4, Reinforced",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-1-49","Concrete Ditch Pavement, 6, Reinforced",null,"SY",null,null,0,null,0,null,0.433778,null,0.106889]
[null,"0524-2-1","Concrete Slope Pavement, NR, 3\"",null,"SY",null,null,0,null,0,null,0.650667,null,0]
[null,"0524-2-2","Concrete Slope Pavement, NR, 4\"",null,"SY",null,null,0,null,0,null,0.650667,null,0]
[null,"0524-2-4","Concrete Slope Pavement, NR, 6\"",null,"SY",null,null,0,null,0,null,0.650667,null,0]
[null,"0524-2-29","Concrete Slope Pavement, NR, 4\", Reinforced",null,"SY",null,null,0,null,0,null,0.650667,null,0]
[null,"0524-2-49","Concrete Slope Pavement, NR, 6\", Reinforced",null,"SY",null,null,null,null,0,null,0.650667,null,0]
[null,"0570-1-1","Performance Turf",null,"SY",null,null,0,null,0,null,1.857E-2,null,5.1000000000000004E-3]
[null,"0570-1-2","Performance Sod",null,"SY",null,null,{"$f":"ROUND(F902*L902,0)","v":0},null,{"$f":"ROUND(F902*N902,0)","v":0},null,1.857E-2,null,5.1000000000000004E-3]
[null,"0570-1-3","Performance Turf, Sod and Soil-Shoulder Treatment Index 570-010",null,"SY",null,null,{"$f":"ROUND(F903*L903,0)","v":0},null,{"$f":"ROUND(F903*N903,0)","v":0},null,1.857E-2,null,5.1000000000000004E-3]
[null,"Updated 12-10-2019",null,null,"TOTAL (GALLONS)",null,null,{"$f":"SUM(H13:H902)","v":0},null,{"$f":"SUM(J13:J902)","v":0},null,"MONTHLY MONETARY AMOUNT"]
[null,"* Quantity for LS pay items = Total Quantity of Secondary unit X % of work completed",null,null,"INDEX DIFFERENCE",null,null,{"$f":"IF((L6*1.05)<L8,L8-(L6*1.05),IF((L6*0.95)>L8,L8-(L6*0.95),0.00000000001))","v":9.9999999999999994E-12},null,{"$f":"IF((N6*1.05)<N8,N8-(N6*1.05),IF((N6*0.95)>N8,N8-(N6*0.95),0.00000000001))","v":9.9999999999999994E-12},null,{"$f":"IF((H904*H905)=0,0.000000001,H904*H905)","v":1.0000000000000001E-9},null,{"$f":"IF((J904*J905)=0,0.000000001,J904*J905)","v":1.0000000000000001E-9}]
[]
[]
["I certify that, based on my personal knowledge and well-founded belief following my own reasonable investigation, the gallons (metric tons and liters) represented by this Certification are true and correct."]
["* Calculations based on Specifications."]
[]
[]
[]
[null,null,null,null,null,null,null," (Name of Company and email address)"]
[null,"Updated 12-10-2019"]
[null,"0285-745"]
[null,"0285-746"]
[null,"Updated 11-05-2019"]
[null,"0285-743"]
[null,"0285-744"]
[null,"0430885-30"]
[null,"Updated 8-06-2019"]
[null,"0285-742"]
[null,"0327-70-46"]
[null,"0425-1921"]
[null,"0425-1922"]
[null,"0425-1923"]
[null,"0425-1924"]
[null,"0425-1925"]
[null,"Updated 6-06-2019"]
[null,"0285-741"]
[null,"0455-34-125"]
[null,"Updated 5-09-2019"]
[null,"0285-740"]
[null,"0430-175-199"]
[null,"Updated 4-08-2019"]
[null,"0285-739"]
[null,"0450-8-31"]
[null,"Updated 3-11-2019"]
[null,"0285-738"]
[null,"0407-1-11"]
[null,"0407-1-21"]
[null,"0425-1795"]
[null,"0521-9-1"]
[null,"Updated 2-13-2019"]
[null,"0350-3-6"]
[null,"0425-1785"]
[null,"0520-5-52"]
[null,"Updated 1-07-2019"]
[null,"0285-736"]
[null,"0285-737"]
[null,"0570-1-3"]
[null,"Updated 11-05-2018"]
[null,"0425-1782"]
[null,"0521-72-42"]
[null,"0521-72-44"]
[null,"Updated 10-03-2018"]
[null,"0285-735"]
[null,"Updated 09-06-2018"]
[null,"0425-1781"]
[null,"0425-1783"]
[null,"0425-1791"]
[null,"0425-1792"]
[null,"0425-1793"]
[null,"0425-1799"]
[null,"0450-8-32"]
[null,"0521-72-60"]
[null,"0521-72-61"]
[null,"Updated 08-06-2018"]
[null,"0521-5-22"]
[null,"0521-8-8"]
[null,"0521-72-41"]
[null,"Updated 07-06-2018"]
[null,"0450-8-14"]
[null,"0521-5-14"]
[null,"0521-72-24"]
[null,"Updated 06-06-2018"]
[null,"0285-734"]
[null,"0521-72-43"]
[null,"Updated 05-07-2018"]
[null,"0430885-24"]
[null,"0430886-24"]
[null,"Updated 03-05-2018"]
[null,"0285-733"]
[null,"0425-1482"]
[null,"0430-886-36"]
[null,"0521-72-27"]
[null,"Updated 02-05-2018"]
[null,"0430-886-60"]
[null,"0450-8-11"]
[null,"0521-72-56"]
[null,"Updated 01-08-2018"]
[null,"   0285-732"]
[null,"   0521-72-40"]
[null,"Updated 11-06-2017"]
[null,"   0120-1-900"]
[null,"   0120-4-900"]
[null,"   0120-6-900"]
[null,"   0160-4-900"]
[null,"   0285-701-900"]
[null,"   0285-709-900"]
[null,"   0521-1-11"]
[null,"   0521-1-12"]
[null,"   0521-1-13"]
[null,"   0521-1-14"]
[null,"Updated 09-06-2017"]
[null,"0334-1-59"]
[null,"0460-94"]
[null,"0521-8-7"]
[null,"0521-8-11"]
[null,"Updated 08-03-2017"]
[null,"0285-731"]
[null,"Updated 07-14-2017"]
[null,"0285-730"]
[null,"0327-70-45"]
[null,"Updated 06-07-2017"]
[null,"0337-7-91"]
[null,"0337-7-92"]
[null,"0521-5-12"]
[null,"Updated 05-08-2017"]
[null,"0285-722"]
[null,"0350-3-15"]
[null,"0415-2-4"]
[null,"0415-2-5"]
[null,"0415-2-9"]
[null,"Updated 04-10-2017"]
[null,"0327-70-44"]
[null,"Updated 03-06-2017"]
[null,"0350-3-14"]
[null,"Updated 02-06-2017"]
[null,"0337-7-80"]
[null,"0337-7-81"]
[null,"0337-7-82"]
[null,"0337-7-83"]
[null,"0337-7-85"]
[null,"0337-7-88"]
[null,"Updated 12-13-2016"]
[null,"0450-8-13"]
[null,"0450-8-33"]
[null,"Updated 11-06-2016"]
[null,"0334-1-58"]
[null,"0337-7-26"]
[null,"0337-7-94"]
[null,"Updated 10-06-2016"]
[null,"0110-4-10"]
[null,"0407-1-52"]
[null,"0430-885-12"]
[null,"0430-885-18"]
[null,"0430-885-36"]
[null,"0430-885-42"]
[null,"0430-885-48"]
[null,"0430-885-60"]
[null,"0444-74-1"]
[null,"0444-74-2"]
[null,"0455-34-25"]
[null,"0455-143-25"]
[null,"Updated 09-06-2016"]
[null,"0110-4-3"]
[null,"0110-4-4"]
[null,"0110-4-5"]
[null,"0110-4-6"]
[null,"0110-4-7"]
[null,"0110-4-11"]
[null,"0110-4-12"]
[null,"0110-4-13"]
[null,"0110-4-15"]
[null,"0110-4-16"]
[null,"0110-4-17"]
[null,"0334-1-52"]
[null,"0334-1-53"]
[null,"0334-1-54"]
[null,"0334-1-55"]
[null,"0334-1-56"]
[null,"0334-1-57"]
[null,"0337-7-25"]
[null,"0337-7-90"]
[null,"0337-7-93"]
[null,"0430-611-023"]
[null,"Updated 08-05-2016"]
[null,"0455-14-23"]
[null,"0521-5-13"]
[null,"Updated 07-01-2016"]
[null,"0430-613-229"]
[null,"Updated 06-06-2016"]
[null,"0450-8-23"]
[null,"0450-8-24"]
[null,"Updated 03-08-2016"]
[null,"0400-4-47"]
[null,"0425-3-62"]
[null,"0450-8-12"]
[null,"Updated 02-16-2016"]
[null,"0400-4-40"]
[null,"0400-4-6"]
[null,"Updated 02-09-2016"]
[null,"0350-30-5"]
[null,"0450-8-21"]
[null,"Updated 01-25-2016"]
[null,"0455-35-12"]
[null,"0455-35-13"]
[null,"Updated 12-02-2015"]
[null,"0400-8-4"]
[null,"0450-3-33"]
[null,"0455-35-10"]
[null,"0455-35-11"]
[null,"0521-8-6"]
[null,"Updated 11-01-2015"]
[null,"0455-14-24"]
[null,"0455-34-23"]
[null,"0455-143-23"]
[null,"Updated 10-05-2015"]
[null,"0327-70-42"]
[null,"0455-143-103"]
[null,"0455-143-105"]
[null,"0455-143-203"]
[null,"0455-143-105"]
[null,"Updated 08-05-2015"]
[null,"0450-4-15"]
[null,"0450-7-6"]
[null,"0455-34-103"]
[null,"0455-34-105"]
[null,"0455-34-106"]
[null,"0455-34-107"]
[null,"0455-34-120"]
[null,"0455-34-121"]
[null,"0455-34-203"]
[null,"0455-34-205"]
[null,"0455-34-206"]
[null,"0455-34-207"]

{"sheet":"Sheet2","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Instructions - Pay Item adj's","index":4,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":true,"merged":[[21,0,21,1],[24,0,25,0],[26,0,27,0],[25,2,25,3]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Change the code"]
["Step 1","Open the Microsoft Visual Basic Window (ALT+F11)"]
["Step 2:","Open the code window for Sheet 1 (Setup)"]
["Step 3:","Change the values MainFormRowVALUE and TemplateRowVALUE to the number of pay items + 1. "]
[null,"i.e. For the range of B13:N64, there are 52 items + 1, makes the correct one be 53 for the value.","Adjust the \"Template\" worksheet's range"]
["Step 4:","Change the ranges MainFormRANGE and TemplateRANGE to match the range on the \"FuelWS\" sheet","Step 5: ","Unhide the Template worksheet"]
[null,"i.e. \"B13:N64\" -- First cell (B13), Last Cell (N64) ; Last cell is  the one you'll be changing to match the last row.","Step 6:","Add or remove rows to match the number of rows in the \"FuelWS\" worksheet"]

{"sheet":"Template","index":5,"n_rows":66,"n_cols":14,"rows_kept":66,"cut":false,"hidden":true,"merged":[[65,2,65,3],[35,2,35,3],[9,4,11,4],[14,2,14,3],[31,2,31,3],[34,2,34,3],[65,4,65,5],[23,2,23,3],[64,4,64,5],[39,2,39,3],[9,13,11,14],[9,11,11,12],[21,2,21,3],[20,2,20,3],[19,2,19,3],[18,2,18,3],[9,9,11,10],[9,7,11,8],[9,5,11,6],[1,2,1,11],[2,2,2,11],[38,2,38,3],[7,3,7,4],[15,2,15,3],[3,3,3,4],[16,2,16,3],[27,2,27,3],[5,3,5,4],[9,2,11,3],[22,2,22,3],[17,2,17,3],[29,2,29,3],[28,2,28,3],[24,2,24,3],[64,11,64,14],[30,2,30,3],[63,2,63,3],[42,2,42,3],[62,2,62,3],[36,2,36,3],[40,2,40,3],[32,2,32,3],[64,2,64,3],[43,2,43,3],[37,2,37,3],[41,2,41,3],[33,2,33,3],[9,1,11,1],[13,2,13,3],[25,2,25,3],[26,2,26,3],[12,2,12,3]]}
[]
[null,null,"CONTRACTOR'S ESTIMATED FUEL WORKSHEET"]
[null,null,"(DESIGN BUILD AND LUMP SUM PROJECTS)"]
[null,"CONTRACTOR:",{"$f":"ContractorName","v":0},"DATE FROM:",null,{"$f":"DateFrom","v":"00:00:00"},null,null,null,"MONTH / YEAR",null,"GASOLINE INDEX",null,"DIESEL INDEX"]
[]
[null,"WORKSHEET NO.:",{"$f":"CertificationNumber","v":0},"DATE TO:",null,{"$f":"DateTo","v":"00:00:00"},null,"BASE INDEX:",null,{"$f":"BaseIndexMonth","v":"00:00:00"},null,{"$f":"GasolineBaseIndex","v":0},null,{"$f":"DieselBaseIndex","v":0}]
[]
[null,"FINANCIAL PROJECT ID:",{"$f":"FinancialIDNumber","v":0},"CONTRACT NO.:",null,{"$f":"ContractNumber","v":0},null,"CURRENT INDEX:",null,{"$f":"CurrentIndexMonth","v":"00:00:00"},null,{"$f":"GasolineCurrentIndex","v":0},null,{"$f":"DieselCurrentIndex","v":0}]
[]
[null,"PAY ITEM NUMBER(S)","ITEM DESCRIPTION",null,"UNIT","QUANTITY",null,"GASOLINE\n(GALLONS)",null,"DIESEL\n(GALLONS)",null,"GASOLINE\nFACTOR",null,"DIESEL\nFACTOR"]
[]
[]
[null,null,null,null,null,null,null,{"$f":"ROUND(F13*L13,0)","v":0},null,{"$f":"ROUND(F13*N13,0)","v":0}]
[null,null,null,null,null,null,null,{"$f":"ROUND(F14*L14,0)","v":0},null,{"$f":"ROUND(F14*N14,0)","v":0}]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,{"$f":"ROUND(F45*L45,0)","v":0},null,{"$f":"ROUND(F45*N45,0)","v":0}]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,null,null,null,0,null,0]
[null,null,null,null,"TOTAL (GALLONS)",null,null,{"$f":"SUM(H13:H64)","v":0},null,{"$f":"SUM(J13:J64)","v":0},null,"MONTHLY MONETARY AMOUNT"]
[null,null,null,null,"INDEX DIFFERENCE",null,null,{"$f":"IF((L6*1.05)<L8,L8-(L6*1.05),IF((L6*0.95)>L8,L8-(L6*0.95),0.00000000001))","v":9.9999999999999994E-12},null,{"$f":"IF((N6*1.05)<N8,N8-(N6*1.05),IF((N6*0.95)>N8,N8-(N6*0.95),0.00000000001))","v":9.9999999999999994E-12},null,{"$f":"IF((H65*H66)=0,0.000000001,H65*H66)","v":1.0000000000000001E-9},null,{"$f":"IF((J65*J66)=0,0.000000001,J65*J66)","v":1.0000000000000001E-9}]

{"sheet":"Accuracy","index":6,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":true,"merged":[[2,2,2,3],[2,7,2,9],[28,1,28,4],[14,2,14,3],[14,7,14,9]]}
[]
[]
[null,null,"Pay Item Accuracy Table",null,null,null,null,"Pay Item Units Table"]
[]
[null,null,"Rounding Display","Round Function",null,null,null,"Units","Directory Name","Accuracy"]
[null,null,null,"Value",null,null,null,null,null,"(Decimal Places)"]
[]
[null,null,1E-3,3,null,null,null,"English","eng","1"]
[null,null,0.01,2,null,null,null,"Metric","met","1"]
[null,null,0.1,1]
[null,null,1,0]
[]
[]
[]
[null,null,"Area Conversion Table",null,null,null,null,"Weight/Volume Units Table"]
[]
[null,null,"Pay Item Units","Conversion Factor",null,null,null,"Units","Weight","Volume"]
[]
[null,null,"AC",43560,null,null,null,"CY",null,"(CY)"]
[null,null,"HA",10000,null,null,null,"GA",null,"(GA)"]
[null,null,"M2",1,null,null,null,"KG","(KG)"]
[null,null,"SF",1,null,null,null,"KL",null,"(KL)"]
[null,null,"SY",9,null,null,null,"LB","(LB)"]
[null,null,null,null,null,null,null,"LI",null,"(LI)"]
[null,null,null,null,null,null,null,"MG",null,"(MG)"]
[null,null,null,null,null,null,null,"MT","(MT)"]
[null,null,null,null,null,null,null,"M3",null,"(M3)"]
[null,null,null,null,null,null,null,"TN","(TN)"]
[null,"NOTE: Do Not Change"]

{"sheet":"FuelFactors","index":7,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":true,"merged":[[2,4,2,7]]}
[]
[]
[null,null,"English or Metric","English or Metric","English"]
[null,null,"Pay Item Number(s)","Description","Unit","Gasoline ","Diesel ","Accuracy"]
[null,null,null,null,null,"Factor","Factor"]
[]
[null,null,"0110-1-1","Clearing & Grubbing","LS/AC",32,45.64,"1"]
[null,null,"0120-1","Regular Excavation","CY",2.8E-3,0.20150000000000001,"1"]
[null,null,"0120-2-2","Borrow Excavation","CY",3.8999999999999998E-3,0.44409999999999999,"1"]
[null,null,"0120-3","Lateral Ditch Excavation","CY",9.9999999999999994E-12,5.33E-2,"1"]
[null,null,"0120-4 to 120-5","Subsoil or Channel Excavation","CY",4.3E-3,0.27879999999999999,"1"]
[null,null,"0120-6","Embankment","CY",3.4099999999999998E-2,0.51749999999999996,"1"]
[null,null,"0160-4","Type B Stabilization","SY",3.0599999999999999E-2,0.1196,"1"]
[null,null,"0162","Soil Layer","SY",9.9999999999999994E-12,6.0000000000000001E-3,"1"]
[null,null,"0285-701 to 0285-708","Base Optional (Group 01 to 08) ","SY",5.6007000000000001E-2,0.215614,"1"]
[null,null,"0285-709 to 0285-715","Base Optional (Group 09 to 15) ","SY",9.2254000000000003E-2,0.43591600000000003,"1"]
[null,null,"0285-701 to 0285-708 (Asph)","Base Superpave Type 12.5  (Asphalt Only)","SY",4.0149999999999998E-2,0.97328800000000004,"1"]
[null,null,"0285-709 to 0285-715 (Asph)","Base Superpave Type 12.5  (Asphalt Only)","SY",6.6000000000000003E-2,1.5999570000000001,"1"]
[null,null,"0286-1","Turnout Construction","SY",2.64E-2,0.6925,"1"]
[null,null,"0286-2","Turnout Construction","TN",0.17599999999999999,4.6220109999999996,"1"]
[null,null,"0327-70-1 to 0327-70-13","Mill Existing Asphalt Pavement","SY",2.7969000000000001E-2,9.1162000000000007E-2,"1"]
[null,null,"0327-70-14 to 0327-70-25","Mill Existing Asphalt Pavement","SY",4.1224999999999998E-2,0.13389499999999999,"1"]
[null,null,"0334-","Superpave Asphalt Concrete","TN",0.17599999999999999,4.6220109999999996,"1"]
[null,null,"0337-","Asphalt Concrete Friction Course (Rubber)","TN",0.17599999999999999,4.6220109999999996,"1"]
[null,null,"0339-1","Miscellaneous Asphalt Pavement","TN",0.17599999999999999,4.6220109999999996,"1"]
[null,null,"0350-1 to 0350-2","Cement Concrete Pavement, Plain","SY",0.12562699999999999,0.28075800000000001,"1"]
[null,null,"0400-1- to 0400-4-","Concrete Class I to IV","CY",0.25506699999999999,1.8677330000000001,"1"]
[null,null,"0400-8-","Concrete Class V","CY",0.25714999999999999,1.8555999999999999,"1"]
[null,null,"0410-70-","Precast Concrete Box Culvert","LF",0.26340000000000002,3.2593000000000001,"1"]
[null,null,"0415-1-","Reinforcing Steel","LB",9.9999999999999994E-12,1.3110000000000001E-3,"1"]
[null,null,"0425-1- to 0425-3-","Drainage Inlets, Manholes or Junction Boxes","EA",1.3169999999999999,7.9226000000000001,"1"]
[null,null,"0430-171- to 0430-174-","Pipe Concrete Culvert","LF",0.16947799999999999,0.56260399999999999,"1"]
[null,null,"0430-721-","Pipe Concrete Culvert","LF",0.16947799999999999,0.56260399999999999,"1"]
[null,null,"0450-1-","Prestressed Beams","LF",3.5099999999999999E-2,0.86040000000000005,"1"]
[null,null,"0450-3-","Prestressed Slabs","LF",3.5099999999999999E-2,0.86780000000000002,"1"]
[null,null,"0450-4-","Prestressed Beams","LF",3.5099999999999999E-2,0.86040000000000005,"1"]
[null,null,"0455-14- to 0455-35-","Piling (Prestressed Concrete)","LF",4.6800000000000001E-2,0.20080000000000001,"1"]
[null,null,"0455-88-","Drilled Shaft","LF",2.2810000000000001,5.5301,"1"]
[null,null,"0455-143- to 0455-144-","Test Pile","LF",4.6800000000000001E-2,0.20080000000000001,"1"]
[null,null,"0460-1-","Structural Steel, Rehabilitation","LB",6.0000000000000002E-5,1.65E-3,"1"]
[null,null,"0460-2-","Structural Steel, New Construction","LS/LB",6.0000000000000002E-5,1.65E-3,"1"]
[null,null,"0460-6","Ladders & Platforms","LB",6.0000000000000002E-5,1.65E-3,"1"]
[null,null,"0460-95","Structural Steel Repair","LB",6.0000000000000002E-5,1.65E-3,"1"]
[null,null,"0520-1- to 0520-7","Concrete Curb & Gutter, Traffic Separator, etc.","LF",9.9999999999999994E-12,0.180531,"1"]
[null,null,"0521-","Barrier Wall Concrete","LF",1.84E-2,0.15989999999999999,"1"]
[null,null,"0522-","Conc Sidewalk","SY",9.9999999999999994E-12,0.28070000000000001,"1"]
[null,null,"0524-","Concrete Ditch or Slope Pavement","SY",0.36,0.16900000000000001,"1"]
[null,null,"0570-1","Performance Turf","SY",0.01,9.9999999999999994E-12,"1"]