{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["CRF","Control Elements"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":11,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CRF","index":0,"n_rows":156,"n_cols":35,"rows_kept":156,"cut":false,"hidden":false,"merged":[[141,0,141,34],[139,0,139,34],[142,0,142,34],[4,25,5,25],[4,26,5,26],[4,27,5,27],[4,33,5,33],[4,34,5,34],[4,28,5,28],[4,29,5,29],[4,30,5,30],[4,31,5,31],[4,32,5,32],[140,0,140,34],[1,0,1,34],[2,0,2,34],[3,1,3,33],[4,2,4,15],[4,0,5,0],[4,1,5,1],[4,16,5,16],[4,17,5,17],[4,18,5,18],[4,19,5,19],[4,20,5,20],[4,21,5,21],[4,22,5,22],[4,23,5,23],[4,24,5,24]]}
[null,"To filter:  Select X from the drop-down arrows:"]
["Crash Reduction Factors (as of 02/14/2014)               "]
["Florida Department of Transportation               "]
[null,"Note:  Use of CRFs based on less than 5 projects (Column C) are not recommended for use in B/C analysis.  Positive CRFs imply reduced crashes.  Negative CRFs imply increased crashes.            "]
["ID","Improvement","Potential Controlling Criteria Application",null,null,null,null,null,null,null,null,null,null,null,null,null,"Number of Projects","Total","Fatal","Injury","PDO","Urban","Rural","Night","Day","Rear-End","Angle","Left-Turn","Right-Turn","Sideswipe","Fixed-Object","Head-On","Pedestrian","Ran-Off-Road","Wet Surface"]
[null,null,"DS","LW","SW","BW","HA","SE","VA","G","SSD","CS","VC","HC","SC","Other"]
[1,"New signal at channelized intersection",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,31,12,15,20,-1,13,7,4,16,-51,53,16,70,10,-40,53,-90,-90,20]
[2,"New signal at non-channelized intersection",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,11,15,58,15,14,20,-27,21,13,-5,11,34,23,23,51,-46,13,26,11]
[3,"Add signal and channelization",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,19,19,-8,25,13,17,21,-41,31,-8,40,50,26,-16,-3,48,58,51,34]
[4,"Modify signal at channelized intersection",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,7,11,null,31,-18,11,null,-13,18,29,20,17,7,-4,-272,-272,7,-86,22]
[5,"Modify signal at non-channelized intersection",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,2,-99,-23,-118,-85,38,-141,-126,-73,-48,-94,-188,100,-23,38,null,null,null,-48]
[6,"Modify both signal and channelization",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,15,24,50,33,13,25,-20,7,29,6,30,66,-4,4,4,-59,34,-164,33]
[7,"Modify signal and add channelization",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,10,28,-87,27,29,28,30,-1,35,11,37,49,25,-42,-20,-87,null,38,-17]
[8,"Remove signal",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[9,"Add flashing warning signal (signalization)",null,null,null,null,"x",null,"x",null,"x",null,null,null,null,null,4,-2,100,-37,28,null,-2,59,-22,80,-30,-117,100,-63,100,null,null,100,46]
[10,"Interconnect traffic signals","x",null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[11,"New LT channelization w/ LT phase (signalized)","x",null,null,null,null,null,null,null,null,null,null,null,null,null,9,17,59,36,-9,16,44,16,19,5,16,50,-42,12,-1,15,29,68,18]
[12,"New LT channelization w/o LT phase (signalized)","x",null,null,null,null,null,null,null,null,null,null,null,null,null,10,31,79,35,26,31,39,33,30,18,46,61,42,39,-26,38,41,12,49]
[13,"New LT channelization (nonsignalized intersection)","x",null,null,null,null,null,null,null,null,null,null,null,null,null,46,3,61,9,-6,-6,20,-26,9,-5,7,24,42,1,-19,-26,6,0,21]
[14,"Modify intersection at signalized intersection",null,null,null,null,"x",null,null,null,"x",null,null,"x",null,null,28,6,-24,13,0,5,78,1,8,7,10,28,11,3,21,-9,16,24,18]
[15,"Modify intersection at non-signalized intersection",null,null,null,null,"x",null,null,null,"x",null,null,"x",null,null,5,18,66,32,6,18,100,13,15,10,25,59,43,31,-53,39,-2,-2,17]
[16,"Modify channelization and add signal",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,2,22,null,21,22,22,null,-131,18,11,16,39,33,-6,58,-68,16,-26,5]
[17,"Increase storage lane",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",8,11,-76,15,9,20,-10,-9,17,0,8,15,-36,7,1,-68,17,-6,17]
[18,"Add turn bay",null,"x","x",null,null,null,"x",null,"x",null,null,null,null,null,8,10,52,16,-1,10,10,1,11,5,6,21,36,20,-222,-190,null,36,48]
[19,"Add right turn","x","x","x",null,null,null,null,null,null,null,null,null,null,null,8,9,67,9,8,0,52,-6,3,11,16,37,1,-20,-39,-33,-49,100,16]
[20,"Add LT (T-intersection)","x","x","x",null,null,null,null,null,null,null,null,null,null,null,3,42,9,56,31,42,43,-39,61,37,84,84,-81,55,-55,100,null,48,-81]
[21,"Add LT (Y-intersection)","x","x","x",null,null,null,null,null,null,null,null,null,null,null,1,42,-118,53,31,42,null,24,56,52,48,84,46,17,32,69,-118,27,64]
[22,"Add 2nd LT lane in same direction as existing",null,"x","x",null,null,null,null,null,null,null,null,null,null,"x",15,4,0,13,-3,1,92,0,2,1,22,30,45,-33,28,-135,-25,13,15]
[23,"Guardrail at bridges end",null,null,null,"x",null,null,null,null,null,null,null,"x",null,null,0]
[24,"Guardrail at steep embankments",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,3,-5,-3,3,-16,-2,-19,-63,2,3,-184,-55,null,74,-120,100,null,5,-9]
[25,"Guardrail at steep embankments with curve",null,"x","x",null,null,"x",null,null,null,null,null,"x",null,null,1,-256,null,-78,null,null,-256,null,-167,null,null,null,null,100,null,null,null,null,11]
[26,"Guardrail at roadside obstacles (piers, sign posts, poles, etc.)",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,1,52,null,60,37,52,null,27,62,44,100,null,null,68,37,100,100,null,54]
[27,"Guardrail end treatments",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,0]
[28,"Guardrail relocation",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,0]
[29,"Guardrail removal",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,0]
[30,"Add painted median",null,"x","x",null,null,null,null,null,null,null,null,null,null,"x",2,43,78,43,40,null,43,-273,25,33,14,68,66,62,-72,57,83,-15,39]
[31,"Add raised median",null,"x","x",null,null,null,null,null,null,null,null,null,null,"x",18,20,38,19,20,20,null,22,19,2,29,48,23,41,-2,45,22,-37,27]
[32,"Increase median width",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,4,-2,-12,0,-3,-10,100,-19,3,3,-43,5,3,-28,30,-699,-224,60,45]
[33,"Add two-way LT lanes","x","x","x",null,null,null,null,null,null,null,null,null,null,null,12,41,35,45,39,40,44,33,44,58,32,36,32,38,34,18,-24,27,24]
[34,"Install concrete median barrier",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,1,-37,56,-27,-46,-37,null,-71,-36,-46,-407,56,94,29,-112,9,-58,-73,-48]
[35,"Install double sided guardrail on wider median",null,"x","x",null,null,null,null,null,null,null,null,"x",null,null,12,-16,33,1,-38,-29,1,-15,-17,3,-4,2,null,19,-83,61,-96,28,-54]
[36,"Install attenuator type (IBC) barrier",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,0]
[37,"Upgrade to concrete median barrier",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,0]
[38,"Upgrade to attenuator barrier",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,0]
[39,"Pavement deslicking",null,null,null,null,null,null,null,null,null,"x","x",null,null,null,4,-3,-30,-13,2,-2,-20,-34,3,17,-24,-7,8,-43,8,-399,35,-127,30]
[40,"Skid Hazard overlay",null,null,null,null,null,null,null,null,null,"x","x",null,null,null,95,-6,-53,-5,-6,-5,-19,-11,-3,2,-35,0,5,-11,-9,-19,-13,-7,18]
[41,"Pavement grooving",null,null,null,null,null,null,null,null,null,"x","x",null,null,null,0]
[42,"Eliminate parking",null,"x","x",null,null,null,null,null,"x",null,null,null,"x",null,4,12,100,11,12,12,null,8,13,2,29,32,46,25,14,13,63,null,26]
[43,"Change two-way operation to one-way",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,0]
[44,"Prohibit turns",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,2,-190,100,-99,-309,-190,null,-43,-360,-198,-138,null,null,null,-19,-19,-19,null,-99]
[45,"Modify speed limit (increase or decrease)","x",null,null,null,null,"x","x",null,"x",null,null,null,"x",null,1,52,56,50,53,null,52,null,54,-18,75,85,null,71,56,null,null,100,78]
[46,"Delineation of right edge lines",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,0]
[47,"Delineation of painted median edge lines",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,1,-76,null,-18,-155,-76,null,-65,-85,-85,7,-85,null,31,-410]
[48,"Centerline striping",null,"x",null,null,null,null,null,null,null,null,null,null,null,null,0]
[49,"Delineation of no passing stripes",null,"x",null,null,"x",null,"x",null,"x",null,null,null,null,null,0]
[50,"Delineation of reflectorized guide markers",null,"x","x",null,"x",null,null,null,null,null,null,null,null,null,0]
[51,"Delineation of reflectorized raised pavement markers (center line)",null,"x",null,null,"x",null,null,null,null,null,null,null,null,null,1,10,23,11,5,null,21,16,3,7,7,-62,100,81,-36,38,100,25,7]
[52,"Delineation of general pavement markings (stop bar, ped. crossing, code 46-51)",null,"x","x",null,null,null,null,null,"x",null,null,null,null,null,0]
[53,"Delineation of guide posts on curves",null,null,null,null,"x","x",null,null,null,null,null,null,null,null,0]
[54,"Intersection delineation",null,"x",null,null,"x",null,null,null,"x",null,null,null,null,null,0]
[55,"Curve warning Signing","x",null,null,null,"x","x",null,null,null,null,null,null,null,null,2,35,null,6,49,44,-306,56,21,72,-2,32,null,49,49,-2,null,null,-19]
[56,"Chevrons Signing","x",null,null,null,"x","x",null,null,null,null,null,null,null,null,1,30,null,12,63,null,30,-120,78,-120,null,100,null,100,-65,100,100,45,-120]
[57,"All-way stops Signing",null,null,null,null,null,null,null,null,"x",null,null,null,null,null,0]
[58,"Overhead directional (where to turn) Signing",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",3,-7,100,-9,-5,-7,null,-17,-4,-15,16,9,41,14,-13,-383,-45,null,-11]
[59,"Roadside directional (where to turn) Signing",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[60,"Overhead lane designation Signing",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[61,"Minor leg stop control Signing",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,0]
[62,"Yield sign",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,0]
[63,"Advanced warning signs",null,null,null,"x","x","x","x","x","x",null,"x",null,"x","x",1,60,null,60,null,null,60,null,60,null,null,100]
[64,"Intersection directional or warning signs",null,null,null,null,"x",null,null,null,null,null,null,null,null,"x",0]
[65,"New roadway segment lighting",null,null,null,null,null,null,"x",null,"x",null,null,"x",null,null,58,2,23,10,-9,2,26,14,-5,-2,-4,25,20,1,-16,-11,33,16,6]
[66,"Upgrade roadway segment lighting",null,null,null,null,null,null,"x",null,"x",null,null,"x",null,null,7,-12,15,-11,-14,-12,100,0,-18,-22,-27,23,57,-1,-8,-39,-1,12,0]
[67,"New lighting at intersection",null,null,null,null,null,null,"x",null,"x",null,null,"x",null,null,9,-2,5,-11,8,-4,-1,31,-15,-30,-15,9,41,12,24,-42,-279,41,-26]
[68,"Upgrade lighting at intersection",null,null,null,null,null,null,"x",null,"x",null,null,"x",null,null,0]
[70,"Bridge approach lighting",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,1,9,null,-5,21,null,9,null,32,-42,null,null,null,62,37,null,null,-26,24]
[71,"Underpass lighting",null,null,null,null,null,null,null,null,null,null,"x",null,null,null,0]
[72,"Intersection flashers four leg red-yellow",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,2,-59,null,null,100,null,-59,null,36,null,-91,52]
[73,"Intersection flashers three leg red-yellow",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,0]
[74,"Intersection flashers four way red",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-105]
[76,"Advanced warning flashers (curve & intersection)",null,null,null,null,"x","x",null,null,"x",null,null,null,null,null,1]
[77,"Install flashing warning signal (flashing beacon)",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,5,-29,null,-65,-12,-52,23,-111,-11,-80,-55,6,48,11,-48,100,null,29,-46]
[78,"Obstacle Removal/Hazard Mitigation",null,null,null,null,null,null,null,null,null,null,null,"x",null,null,5,25,28,37,5,26,19,33,19,22,37,44,14,4,19,6,-38,61,28]
[79,"Relocate obstacle 30 feet from road",null,null,null,null,null,null,null,null,null,null,null,"x",null,null,0]
[80,"Convert to breakaway",null,null,null,null,null,null,null,null,null,null,null,"x",null,null,0]
[81,"Cushion attenuators",null,null,null,null,null,null,null,null,null,null,null,"x",null,null,0]
[82,"Install guardrail",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,9,-38,43,-9,-77,-57,16,-44,-37,-19,-37,19,100,-32,-82,-49,27,-6,-67]
[83,"Upgrade substandard bridgerail",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,1,25,null,100,-125,25,null,100,-12,null,null,null,null,null,-12]
[84,"Realignment",null,null,null,null,"x",null,"x",null,"x",null,null,null,null,null,3,60,50,71,50,-50,100,33,60,57,100,100,null,null,-200,null,null,null,0]
[85,"Superelevation",null,null,null,null,"x","x",null,null,null,null,null,null,null,null,1]
[86,"Modify/Close median openings","x",null,null,null,null,null,null,null,"x",null,null,null,null,null,27,18,40,26,9,18,92,6,21,6,29,58,25,11,-18,-46,-25,45,20]
[87,"Relocate drives",null,null,null,null,null,"x",null,null,"x",null,null,null,null,"x",0]
[88,"Curtail turning movements",null,null,null,null,null,null,null,null,"x",null,null,null,null,"x",0]
[89,"Increase radii at intersection",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,2,38,100,16,58,null,57,21,44,-5,48,-5,null,null,null,null,100,null,-109]
[90,"Widen travel way",null,"x",null,null,null,"x",null,null,null,null,null,null,null,null,2,-52,27,-31,-66,null,-2,-149,-40,7,-56,-136,-164,-27,-10,45,-10,-147,-65]
[91,"Widen shoulder",null,null,"x",null,null,null,null,null,"x",null,null,null,null,null,1,-9,26,-11,-11,null,16,-845,-18,5,-178,-48,-233,72,-39,-48,null,-78,1]
[92,"Add 4 foot shoulders (bike lane)",null,null,"x",null,null,null,null,null,null,null,null,null,null,null,1,6,null,15,3,6,null,-95,17,-15,-37,57,59,51,-173,null,null,67,-18]
[93,"Construct grade separation",null,null,null,null,"x",null,"x",null,"x",null,null,null,null,"x",0]
[94,"Widen bridge (min. of 6 feet)",null,"x","x","x",null,null,null,null,null,null,null,null,null,null,5,55,-39,19,73,-39,65,7,61,48,-109,54,100,69,51,30,30,79,25]
[95,"Reconstruct road & shoulders",null,"x","x",null,null,"x",null,"x",null,null,null,null,null,null,10,-11,-99,-13,-8,-23,66,-41,-2,-1,-51,-9,9,-10,-35,-43,-29,-73,12]
[96,"Reconstruct curve",null,null,null,null,"x","x",null,null,null,null,null,null,null,null,3,42,100,53,43,40,54,28,53,23,27,58,100,78,48,100,17,64,27]
[97,"Construct interchange",null,null,null,null,"x",null,"x",null,"x",null,null,null,null,null,1,-60,100,-188,-24,null,100,100,-99,-61,null,null,null,-13,-50,null,null,25,-126]
[98,"Lengthen accel/decel lanes","x",null,null,null,null,null,null,null,"x",null,null,null,null,null,1]
[99,"Extend drop lane","x",null,null,null,null,null,null,null,"x",null,null,null,null,null,0]
[100,"Install rumble strips",null,"x","x","x","x","x",null,null,"x",null,null,null,null,null,9,22,50,19,22,4,23,38,7,0,14,17,-56,48,4,36,-56,46,20]
[101,"Flatten side slopes",null,null,"x",null,null,null,null,null,null,null,null,"x",null,null,0]
[102,"Install Accel/Decel lane","x",null,null,null,null,null,null,null,"x",null,null,null,null,null,2,20,100,9,8,null,20,52,10,39,22,-7,null,46,null,null,100,57,-115]
[103,"Upgrade signal and add pedestrian feature",null,null,null,null,null,null,null,null,"x",null,null,null,null,"x",17,-5,10,16,-20,-5,null,-7,-7,-20,-20,19,-9,0,19,-78,0,37,-2]
[104,"Sight distance improvements",null,null,null,null,"x",null,null,null,"x",null,null,null,null,null,3,25,-93,38,10,24,25,61,4,13,49,81,null,52,100,null,null,null,4]
[105,"Minor structures replaced or improved for safety",null,null,null,null,null,null,null,null,null,null,null,"x","x",null,1,14,null,32,-23,14,null,23,5,3,22,45,56,-14,56,100,-17,null,-86]
[106,"Lanes added to travel way",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,4,13,69,18,5,13,null,26,5,-2,35,72,6,-15,-26,-214,-183,53,6]
[107,"Upgraded guardrail",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,1,-22,-46,-16,-33,2,-44,8,-44,-25,-7,-155,-292,29,-85,-370,74,-10,-1]
[108,"Sidewalk construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",15,-11,-9,1,-29,-11,null,2,-19,-16,-11,14,3,-34,-2,43,15,-15,1]
[109,"Over/Under passes for pedestrians and/or bicycles",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",2,37,null,7,67,37,null,31,35,20,100,null,null,57,null,13,null,null,48]
[110,"Fencing or other pedestrian barriers",null,null,null,null,null,null,null,null,null,null,null,"x",null,"x",2,-4,100,11,-43,-4,null,-61,4,3,10,27,100,-107,-12,3,-45,null,1]
[111,"Ramps on existing curbs",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[112,"New bikeway/multi-use path construction",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[113,"Bicycle non-construction improvements",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",0]
[114,"Impact Attenuators",null,null,"x","x",null,null,null,null,null,null,null,"x",null,null,3,2,null,16,-27,2,null,-14,4,-3,-14,45,-36,26,-70,-2,-2,74,2]
[115,"Signing and Pavement Markings",null,"x","x","x",null,"x",null,null,null,"x",null,null,null,null,11,11,1,11,11,11,6,0,13,10,5,20,4,-21,13,23,-14,8,15]
[116,"Install Traffic Calming Features","x",null,null,null,null,null,null,null,null,null,null,null,null,null,2,8,100,3,-16,8,null,13,20,42,36,null,null,42,-132,100,null,71,42]
[117,"Add paved shoulders",null,null,"x",null,null,"x",null,null,null,"x",null,null,null,null,21,5,-6,12,-9,8,2,9,2,-1,-5,22,40,11,-2,-2,24,4,19]
[118,"Add turn lane/s & pavement resurfacing",null,"x","x",null,null,"x",null,null,null,"x",null,null,null,null,6,35,3,47,21,35,null,45,31,49,20,53,51,-15,3,51,3,-46,33]
[119,"Reconstruct bicycle/multi-use path",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",1,37,100,40,33,37,null,64,24,17,38,52,4,61,36,52,null,null,71]
[120,"Construct median, add signal, & pavmnt.resurfacing",null,"x","x",null,null,"x",null,null,null,"x",null,null,null,null,4,9,-104,34,-30,9,null,-6,13,31,4,22,-53,-55,-13,32,null,100,33]
[121,"Reconstruct median/median improvments",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,16,-14,56,-6,-27,-25,40,0,-19,-31,-57,14,13,-27,-5,-10,-26,26,-23]
[122,"Construct LT and RT lanes",null,"x","x",null,null,null,null,null,null,null,null,null,null,null,5,-8,-7,-4,-12,-12,39,5,-8,-1,-76,11,-22,-107,5,-114,20,47,19]
[123,"Paved shoulders & rumble strips",null,"x","x",null,null,"x",null,null,null,"x",null,null,null,null,3,3,69,8,-17,-79,51,-1,11,-38,-57,62,65,-5,-10,25,100,5,24]
[124,"Upgrade traffic signal",null,null,null,null,null,null,null,null,"x",null,"x",null,null,"x",3,16,null,21,12,16,null,20,11,34,14,-27,-45,-31,30,-24,31,null,35]
[125,"Traffic signals, guardrail, signing & lighting",null,null,null,null,null,null,null,null,"x",null,null,"x",null,"x",0]
[126,"Traffic signals, resurfacing, turn lanes, lighting",null,"x","x",null,null,null,"x",null,null,null,null,"x",null,null,4,-51,100,-27,-87,-36,-158,-105,-48,-52,-32,-47,-67,-80,-128,-42,-24,29,-37]
[127,"Resurface, guardrail, signing & pavt. markings",null,"x","x",null,null,"x",null,null,null,"x",null,"x",null,null,1,-23,null,25,-161,-23,null,-112,2,-71,16,76,null,null,100,null,null,-96,-96]
[128,"Add Ped crossing mid-block with signals",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",3,-23,-93,-21,-24,-23,null,-25,-16,-60,-19,null,-286,4,4,null,52,null,-148]
[129,"Add Ped crossing mid-block without signals",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",1,-52,-46,-27,-108,-52,null,-37,-58,-70,-22,19,-191,-154,-240,-122,-73,100,-37]
[130,"Add roundabout to intersection","x",null,null,"x",null,null,null,null,"x",null,null,null,null,null,2,46,100,58,32,46,null,41,47,65,17,76,-90,44,5,-1607,-8,100,66]
[131,"Convert shldr inverted rumble to audible edgeline",null,null,"x",null,null,null,null,null,null,null,null,null,null,null,0]
[132,"New inverted AUDIBLE marking on CL or edgeline",null,"x","x",null,"x","x",null,null,null,"x",null,null,null,null,12,6,4,14,-6,-5,11,3,9,-19,18,35,21,55,15,17,15,40,4]
[133,"Use of ITS safety system device(s)",null,null,null,null,null,null,null,null,null,null,null,null,null,"x",1,-16,null,52,-42,-16,null,-3,-8,-267,31,-3,-106,-158,-3,83,100,null,-106]
[134,"High friction surface treatment (tyregrip, etc.)",null,null,null,null,"x","x",null,"x",null,"x",null,null,null,null,1]
[135,"Modify signal timing and phasing","x",null,null,null,null,null,null,null,null,null,null,null,null,"x",2,14,null,30,-1,14,null,-9,20,-22,31,66,-20,-17,33,100,-141,null,36]
[]
["1. Source of Crash Data: The Department of Highway Safety and Motor Vehicles (DHSMV) is the official custodian of the crash reports. The numbers that DHSMV reports are the official numbers. The Florida Department of Transportation (FDOT) Safety Office maintains its own database with crash data obtained from DHSMV, and conducts analyses based on this data for internal FDOT purposes."]
["2. Use Restrictions: The information on the Traffic Safety Web Portal has been compiled from information collected for the purpose of identifying, evaluating or planning safety enhancements. It is used to develop highway safety construction improvements projects which may be implemented utilizing Federal Aid Highway funds. Any document displaying this notice shall be used only for the purposes deemed appropriate by the Florida Department of Transportation. See Title 23, United States Code, Section 409."]
["3. Crash Reduction Factors Parameters - ID: 465, From Year: Any Year, To Year: 2009, Before Month: 36, Min. Before Month: 12, After Month: 36, Min. After Month: 12"]
[null,null,"DS","-","Design Speed"]
[null,null,"LW","-","Lane Width"]
[null,null,"SW","-","Shoulder Width"]
[null,null,"BW","-","Bridge Width"]
[null,null,"HA","-","Horizontal Alignment"]
[null,null,"SE","-","Superelevation"]
[null,null,"VA","-","Vertical Alignment"]
[null,null,"G","-","Grade"]
[null,null,"SSD","-","Stopping Sight Distance"]
[null,null,"CS","-","Cross Slope"]
[null,null,"VC","-","Vertical Clearance"]
[null,null,"HC","-","Horizontal Clearance"]
[null,null,"SC","-","Structural Capacity"]

{"sheet":"Control Elements","index":1,"n_rows":15,"n_cols":1,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["Control Element"]
["Design Speed"]
["Structural Capacity"]
["Superelevation"]
["Horizontal Clearance"]
["Lane Widths"]
["Vertical Clearance"]
["Horizontal Alignment"]
["Shoulder Width"]
["Grades"]
["Vertical Alignment"]
["Bridge Widths"]
["Cross Slope"]
["Stopping Sight Distance"]
["Other (describe in box below)"]