Structures Design Guidelines | July 2007
8 - Movable Bridges |

## 8.2 Construction Specifications and Design Calculations (01/07) Jan 2007 Requires detailed calculations to be included with 60% submittals. Jan 2006, Per AFR, deleted requirement to use FDOT Standard Specs.

A. Use the “Technical Special Provisions” issued by the Mechanical/Electrical Section of the SDO. Additional specifications may be required.

B. Provide detailed calculations to justify all equipment and systems proposed with the 60% Plans Submittal. Provide catalog cuts or sketches showing centerlines,outlines and dimensions.

C. Submit calculations in an 8˝-inch x 11-inch binder.